{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Tabelle1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":1,"defined_names":1,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabelle1","index":0,"n_rows":573,"n_cols":15,"rows_kept":573,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["BUK und AFKzV",null,"Prüfung von Ausrüstung und Geräten der Feuerwehr"]
[]
["Ausrüstung und Geräte",null,"Prüfung bei bzw. nach",null,"Regelmäßige Prüfung",null,"Rechtsgrundlagen, Prüfgrundsätze"]
[null,null,"einer Benutzung"]
["Schutzkleidung und",null,"vor einer","nach einer","Sicht und ","Belastungs-","UVV ","GUV-G 9102","Norm","Sonstige"]
["Schutzgerät",null,"Übung","Benutzung","Funktion","prüfung",null,"Abschnitt"]
["Chemikalienschutzanzug",null,null,"        x","     jährlich","    jährlich",null,null,"EN 943-2"]
["(Typ 1A oder 1B)",null,null,"       1)","        7)","     1) 6)"]
["Chemikalienschutzoverall",null,null,"        x","     jährlich",null,null,null,"EN 466-1"]
["(Typ 3)",null,null,null,"        1)"]
["Schutzkleidung für die",null,null,null,"     jährlich"]
["spezielle ",null,null,"        x","        6)",null,null,null,"EN 1486"]
["Brandbekämpfung"]
["Warnkleidung",null,null,"        x","     jährlich",null,null,null,"EN 471"]
[{"$nulls":4},"        1)"]
["Wathose",null,null,"        x","     jährlich"]
[{"$nulls":4},"      3) 6)"]
[]
[]
["Chemikalien-",null,null,"        x",{"$nulls":4},"EN 374"]
["schutzhandschuhe",null,null,"      3) 6)"]
["Schnittschutzkleidung",null,null,"        x",{"$nulls":4},"EN 381"]
[null,null,null,"      3) 6)"]
["Rettungsweste",null,"         x","        x","     jährlich",null,"BGR 201",null,"EN 396"]
["manuell und automatisch",{"$nulls":7},"EN 399"]
["Ölschutzkleidung",null,null,"        x","     jährlich",null,null,null,"EN 532"]
["flammenhemmend",null,null,null,"      3) 1)",null,null,null,"EN 533"]
["Gehörschützer",null,null,"        x","     jährlich",null,null,null,"EN 352"]
["(Mehrweg)",null,null,"       1)","        3)"]
["Feuerwehrhelm",null,null,"        x","     jährlich",null,null,null,"EN 443","Merkblatt PSA"]
[null,null,null,"    3) 6) 7)","        1)",{"$nulls":4},"23)"]
["Gesichtsschutz",null,null,"       x","jährlich",null,null,null,"EN 1731","Merkblatt PSA"]
[{"$nulls":4},"        3)",{"$nulls":4},"23)"]
["Feuerschutzhaube",null,null,"        x",{"$nulls":4},"prEN 13911","Merkblatt PSA"]
[null,null,null,"      3) 6)",{"$nulls":5},"23)"]
["Feuerwehrschutzanzug",null,null,"        x","     jährlich",null,null,null,"EN 469","        16)"]
[{"$nulls":9},"Merkblatt PSA"]
[{"$nulls":9},"23)"]
["Ausrüstung und Geräte",null,"Prüfung bei bzw. nach",null,"Regelmäßige Prüfung",null,"Rechtsgrundlagen, Prüfgrundsätze",null,null,"Seite 2"]
[null,null,"einer Benutzung"]
["Schutzkleidung und",null,"vor einer","nach einer","Sicht und ","Belastungs-","UVV ","GUV-G 9102","Norm","Sonstige"]
["Schutzgerät",null,"Übung","Benutzung","Funktion","prüfung",null,"Abschnitt"]
["Feuerwehr-",null,null,"        x",{"$nulls":4},"EN 659","Merkblatt PSA"]
["schutzhandschuhe",null,null,"      3) 6)",{"$nulls":5},"23)"]
["Feuerwehrstiefel",null,null,"        x","     jährlich",null,null,null,"EN 345","Merkblatt PSA",{"$nulls":4}," "]
[null,null,null,"        3)","        1)",null,null,null,"prEN ISO 17250","23)"]
["Feuerwehrbeil",null,null,"        x","     jährlich",null,null,null,"DIN 14924"]
[null,null,null,"        3)","        3)"]
["Atemanschluss",null,"         x","        x"," halbjährlich",null,"GUV-R 190",null,"EN 136","vfdb 0804"]
["(Vollmaske)",null,null,null,"       18) ",null,"BGR 190",null,null,"FwDV 7"]
["Masken/Helm-",null,"         x","        x"," halbjährlich",null,"GUV-R 190",null,null,"vfdb 0804"]
["Kombination",null,null,null,"       18)  ",null,"BGR 190",null,null,"FwDV 7"]
["Pressluftatmer",null,"         x","        x"," halbjährlich","    6 Jahre","GUV-R 190",null,"EN 137","vfdb 0804"]
[{"$nulls":4},"       18)","       4)","BGV 190",null,null,"FwDV 7"]
["Regenerationsgerät",null,"         x","        x","halbjährlich","    6 Jahre","GUV-R 190",null,"EN 145","  vfdb 0804"]
["(Kreislaufgerät)",null,null,"        2)",null,"       4)","BGV 190",null,null,"FwDV 7"]
["Filtergerät",null,"         x","        x","halbjährlich",null,"GUV-R 190",null,"EN 141","vfdb 0804"]
[{"$nulls":4},"      21)",null,"BGV 190",null,null,"FwDV 7"]
["Fluchthaube",null,null,"        x","    jährlich",null,"GUV-R 190",null,"EN 403","vfdb 0804"]
["(Filtergerät mit Haube ...)",null,null,null,"       11) 21)",null,"BGV 190",null,null,"FwDV 7"]
["Atemluftflasche",null,"         x","        x","   monatlich","2 Jahre äußere Prüfung","GUV-R 190",null,"EN 12021","vfdb 0804"]
["(Atemschutzgerät)",null,null,null,"        3)","5 Jahre innere Prüfung","BGV 190",null,"DIN 3171","FwDV 7"]
[{"$nulls":5},"10 Jahre Festigkeitsprüfung","BetrSichV",null,"EN 144"]
["Tauchgerät",null,"         x","        x","   monatlich","    6 Jahre",null,null,"EN 250","vfdb 0803"]
[{"$nulls":5},"     4) 18)",null,null,null,"FwDV 8"]
["Atemluftflasche",null,"         x","        x","   monatlich","    2,5 Jahre innere, äusere u.","BetrSichV",null,"EN 144","vfdb 0803"]
["(Tauchgerät)",{"$nulls":4},"    Gewichtsprüfung",null,null,null,"FwDV 8"]
[{"$nulls":5},"5 Jahre Festigkeitsprüfung"]
["Rettungsgerät",null,"         x","        x","vierteljährlich","   jährlich","GUV-R 1/541",null,"EN 12628","FwDV 8"]
["(spezielle Taucheraustüstung)",null,null,null,"        3)",null,null,null,"EN 1809"]
["Atemluftkompressor",null,null,null,"   monatlich","  halbjährlich","VBG 16",null,"EN 12021","TRG 402"]
["(Verdichter)",{"$nulls":4},"3)","GUV-R 190",null,"EN 1012-1"]
[{"$nulls":6},"BGR 190"]
["Ausrüstung und Geräte",null,"Prüfung bei bzw. nach",null,"Regelmäßige Prüfung",null,"Rechtsgrundlagen, Prüfgrundsätze",null,null,"Seite 3"]
[null,null,"einer Benutzung"]
["Löschgerät",null,"vor einer","nach einer","Sicht und ","Belastungs-","UVV ","GUV-G 9102","Norm","Sonstige"]
[null,null,"Übung","Benutzung","Funktion","prüfung",null,"Abschnitt"]
["Kübelspritze",null,null,"        x","    monatlich",null,null,null,"DIN 14405"]
[]
["Feuerlöscher (tragbar)",null,null,"        x","    2 Jahre",null,"GUV-R 133",null,"DIN 14406-4"]
[null,null,null,"        2)","        2)",null,"BetrSichV",null,"EN 3-5"]
[{"$nulls":6},"GUV-V A1"]
[{"$nulls":6},"BGR 133"]
["Pulverlöschgerät (fahrbar)",null,null,"        x","    2 Jahre","    5 Jahre","GUV-R 133",null,null,"TRB 801"]
[null,null,null,"        2)","        2) ","     4) 19)","BetrSichV"]
[{"$nulls":6},"GUV-V A1"]
[{"$nulls":6},"BGR 133"]
["Schaumlöschgerät ",null,null,"        x","    2 Jahre"]
["(fahrbar)",null,null,"        2)","        2)"]
["Schaummittel",null,null,null,"halbjährlich",null,null,null,"EN 1568"]
[{"$nulls":4},"      21)"]
["CO2-Löschgerät (fahrbar)",null,null,"        x","    2 Jahre","22)","BetrSichV"]
[null,null,null,"        2)","        2)"]
["Geräte zur",null,null,"        x","    jährlich"]
["Schaumerzeugung",null,null,null,"        3)"]
["Druckschläuche",null,null,"        x"," bei jeder"," bei jeder","GUV-V C 53",9,"DIN 14811-1"]
[{"$nulls":4},"  Wäsche","  Wäsche"]
["Formstabile Druckschläuche ",null,null,"        x","   jährlich","   jährlich","GUV-V C 53",10,"EN 1947"]
[null,null,null,"        3)"]
["Druckschläuche",null,null,"        x","   jährlich"," bei jeder","GUV-V C 53",9,"DIN 14811-1","BGR 132"]
["mineralölbeständig",null,null,"        3)","       3)"," Wäsche 3)","GUV-R 132",null,"DIN 14555-12"]
[{"$nulls":6},"BGR 132"]
["Saugschläuche",null,null,"        x","   jährlich","   jährlich","GUV-V C 53",11,"DIN 14810"]
[{"$nulls":8},"ISO 14557"]
["Ansaugschläuche ",null,null,"        x","   jährlich",null,null,null,"DIN 14819"]
[]
["Druck-/Saugschläuche",null,null,"        x","   jährlich","   jährlich","GUV-R 132",null,"DIN 14555-12"]
["chemikalienbeständig",null,null,"        3)"," ","       3)","BGR 132",null,"EN 12115"]
[]
["Ausrüstung und Geräte",null,"Prüfung bei bzw. nach",null,"Regelmäßige Prüfung",null,"Rechtsgrundlagen, Prüfgrundsätze",null,null,"Seite 4"]
[null,null,"einer Benutzung"]
["Löschgerät",null,"vor einer","nach einer","Sicht und ","Belastungs-","UVV ","GUV-G 9102","Norm","Sonstige"]
[null,null,"Übung","Benutzung","Funktion","prüfung",null,"Abschnitt"]
["Wasserführende",null,null,"        x","   jährlich","   jährlich"]
["Armaturen und Zubehör",null,null,"        3)","       3)","       3)"]
["z.B. Strahlrohre"]
["Rettungsgerät",null,"vor einer","nach einer","Sicht und ","Belastungs-","UVV ","GUV-G 9102","Norm","Sonstige"]
[null,null,"Übung","Benutzung","Funktion","prüfung",null,"Abschnitt"]
["Hubrettungsfahrzeug",null,null,"     x","jährlich","jährlich","ZH 1/515",12,"DIN 14701"]
[{"$nulls":4},"2)","2)",null,null,"E DIN EN 14043"]
["Drehleitern mit Handbetrieb",null,null,"     x","jährlich","jährlich",null,14,"DIN 14702"]
[null,null,null," ","2)","2)"]
["Anhängeleitern",null,null,"x","jährlich","jährlich",null,15,"DIN 14703"]
[{"$nulls":4},"2)","2)"]
["Schiebleiter 3-teilig Holz",null,"x","x","jährlich","jährlich","GUV-V D 36",8,"EN 1147","EN 1147 für"]
[{"$nulls":6},"GUV-V C 53",null,null,"alle Leitern"]
[{"$nulls":6},"BGV D 36"]
["Schiebleiter 3-teilig ",null,"x","x","jährlich","jährlich","GUV-V D 36",8,"EN 1147"]
["Leichtmetall",{"$nulls":5},"GUV-V C 53"]
[{"$nulls":6},"BGV D 36"]
["Steckleiter, Holz",null,"x","x","jährlich","jährlich","GUV-V D 36",6,"EN 1147"]
[{"$nulls":6},"GUV-V C 53"]
[{"$nulls":6},"BGV D 36"]
["Steckleiter, Leichtmetall",null,"x","x","jährlich","jährlich","GUV-V D 36",6,"EN 1147"]
[{"$nulls":6},"GUV-V C 53"]
[{"$nulls":6},"BGV D 36"]
["Steckleiter, Einsteckteil",null,"x","x","jährlich",null,"GUV-V D 36",null,"EN 1147"]
[null,null,null,"3)","3)",null,"GUV-V C 53"]
[{"$nulls":6},"BGV D 36"]
["Klappleiter",null,"x","x","jährlich"," ","GUV-V D 36",7,"EN 1147"]
[null,null,null,"3)",null,null,"GUV-V C 53"]
[{"$nulls":6},"BGV D 36"]
["Hakenleiter, Holz",null,"x","x","jährlich","jährlich","GUV-V D 36",5,"EN 1147"]
[{"$nulls":6},"GUV-V C 53"]
[{"$nulls":6},"BGV D 36"]
["Ausrüstung und Geräte",null,"Prüfung bei bzw. nach",null,"Regelmäßige Prüfung",null,"Rechtsgrundlagen, Prüfgrundsätze",null,null,"Seite 5"]
[null,null,"einer Benutzung"]
["Rettungsgerät",null,"vor einer","nach einer","Sicht und ","Belastungs-","UVV ","GUV-G 9102","Norm","Sonstige"]
[null,null,"Übung","Benutzung","Funktion","prüfung",null,"Abschnitt"]
["Hakenleiter, Leichtmetall",null,"x","x","jährlich","jährlich","GUV-V D 36",5,"EN 1147"]
[{"$nulls":6},"GUV-V C 53"]
[{"$nulls":6},"BGV D 36"]
["Strickleiter",null,"x","x","jährlich"]
[null,null,"3)","3)","3)"]
["Multifunktionsleiter",null,"x","x","jährlich","jährlich","BGV D 36",null,"EN 1147"]
[{"$nulls":6},"GUV-V D 36"]
["Sprungtuch",null,"x","x","jährlich"," ","GUV-V C 53","3","DIN 14151 T 1"]
[null,null,"3)"]
[]
["Sprungpolster",null,"x","x1)2)","1) ","1) ","GUV-V C 53","3","DIN 14151 T1-T3"]
[{"$nulls":4},"jährlich","jährlich"]
["Abseilgerät",null,"x","x","jährlich","alle 10 Jahre","GUV-R 198",null,null,"Prüfer"]
[null,null,null,"1),2)",null,"4)","GUV R-199",null,null,"Qualifikation"]
[{"$nulls":6},"BGR 198",null,null,"nach BGG 906"]
[{"$nulls":6},"BGR 199"]
["Rettungstuch",null,"x","x","jährlich",null,null,null,"DIN 13040"]
[null,null,null,"3)","3) 6)"]
["Auffanggurt",null,"x","x","jährlich",null,"GUV-R 198",null,"EN 361"]
[{"$nulls":6},"GUV R-199"]
[{"$nulls":6},"GUV-R 199"]
[null,null,"3)","1) 2)","1) 3)",null,"BGR 198"]
[{"$nulls":6},"BGR 199"]
["Kernmatelstatikseil",null,"x","x","jährlich",null,"GUV-R 198",null,"EN 1891"]
[null,null,"3)","1) 2)","1) 3)",null,"GUV-R 199"]
[{"$nulls":6},"BGR 198"]
[{"$nulls":6},"BGR 199"]
["Kernmanteldynamikseil",null,"x","x","jährlich",null,"GUV-R 198",null,"EN 892"]
[{"$nulls":6},"GUV-R 199"]
[null,null,"3)","1) 2)","1) 3)",null,"BGR 198"]
[{"$nulls":6},"BGR 199"]
["Falldämpfer",null,"x","x","jährlich","Falldämpfer sind Einweggeräte und sind nach einer Belastung durch Sturz sofort"]
[{"$nulls":5},"auszusondern!","GUV-R 198"]
[null,null,null,"1) 2)",null,null,"GUV-R 199",null,"EN 355"]
[{"$nulls":6},"BGR 198"]
[{"$nulls":6},"BGR 199"]
["Ausrüstung und Geräte",null,"Prüfung bei bzw. nach",null,"Regelmäßige Prüfung",null,"Rechtsgrundlagen, Prüfgrundsätze",null,null,"Seite 6"]
[null,null,"einer Benutzung"]
["Rettungsgerät",null,"vor einer","nach einer","Sicht und ","Belastungs-","UVV ","GUV-G 9102","Norm","Sonstige"]
[null,null,"Übung","Benutzung","Funktion","prüfung",null,"Abschnitt"]
["Feuerwehrleine",null,null,"x","jährlich",null,"GUV-V C 53","2","DIN 14920"]
[{"$nulls":6},"GUV-R 199"]
[{"$nulls":6},"GUV-R 199"]
[{"$nulls":6},"BGR 199"]
["Feuerwehr-Haltegurt",null,"x","x","jährlich",null,"GUV-V C 53",1,"EN 358"]
[null,null,"3)","13)",null,null,"GUV-R 199",null,"DIN 14926"]
[{"$nulls":6},"BGR 199"]
["Rettungsboot (RTB 1; RTB 2)",null,"x","x","jährlich",null,"GUV-V D 19",null,"DIN 14961"]
[null,null,null,"3)","1)",null,"BGV D 19"]
["FW Mehrzweckboot",null,"x","x","jährlich",null,"GUV-V D 19",null,"DIN 14961"]
[null,null,null,"3)","1) 3)",null,"BGV D 19"]
["Ausrüstung und Geräte",null,"Prüfung bei bzw. nach",null,"Regelmäßige Prüfung",null,"Rechtsgrundlagen, Prüfgrundsätze",null,null,"Seite 6"]
[null,null,"einer Benutzung"]
[]
[]
[{"$nulls":6},"BGV D 19"]
["Sanitäts- und Wieder-",null,"vor einer","nach einer","Sicht und ","Belastungs-","UVV ","GUV-G 9102","Norm","Sonstige"]
["belebungsgerät",null,"Übung","Benutzung","Funktion","prüfung",null,"Abschnitt"]
["Krankentrage",null,null,"x","jährlich",null,null,null,"DIN 13024","1)"]
[{"$nulls":4},"3)",null,null,null,"T 1 u. T 2"]
["Krankentransporthänge-",null,"x","x","jährlich",null,null,null,"DIN 13023"]
["matte",null,null,null,"3)"]
["Verbandkasten E",null,null,"x","jährlich",null,null,null,"DIN 13169","1)"]
[{"$nulls":4},"3)"]
["Kammerschienen pneu-",null,null,"x","monatlich",{"$nulls":4},"15), 1)"]
["matisch",null,null,null,"3)"]
["Beatmungsgerät",null,null,"x","monatlich",{"$nulls":4},"15), 1)"]
[" (Ambubeutel) "]
["Intubationsbesteck",null,null,"x","monatlich",{"$nulls":4},"1)"]
[null,null,null,"3)","3) 8) 10)"]
["Sekretabsaugpumpe",null,null,"x","monatlich",{"$nulls":4},"15), 1)"]
[null,null,null,"3)","3)"]
["Sauerstoffflasche, med.",null,"x","x","monatlich","Äußere Prüfung 2 J",null,null,null,"BetrSichV"]
[{"$nulls":5},"Innere Prüfung 5 J"]
[{"$nulls":5},"Festigkeitsprüfung 10 J 22)"]
["Beleuchtungs-Signal  ",null,"vor einer","nach einer","Sicht und ","Belastungs-","UVV ","GUV-G 9102","Norm","Sonstige"]
["und Fernmeldegerät",null,"Übung","Benutzung","Funktion","prüfung",null,"Abschnitt"]
["Handscheinwerfer, Ex",null,null,"x","monatlich",null,"GUV-V A 2",null,"EN 50014"]
[null,null,null,"8)","1)",null,"GUV-I 8524"]
[{"$nulls":6},"BGV A 2"]
[]
[]
[]
[]
["Ausrüstung und Geräte",null,"Prüfung bei bzw. nach",null,"Regelmäßige Prüfung",null,"Rechtsgrundlagen, Prüfgrundsätze",null,null,"Seite 7",null," "]
[null,null,"einer Benutzung"]
["Beleuchtungs-Signal  ",null,"vor einer","nach einer","Sicht und ","Belastungs-","UVV ","GUV-G 9102","Norm","Sonstige"]
["und Fernmeldegerät",null,"Übung","Benutzung","Funktion","prüfung",null,"Abschnitt"]
["Kopfscheinwerfer, Ex",null,null,"x","monatlich",null,"GUV-V A 2",null,"EN 50014"]
[null,null,null,"8)","1)",null,"GUV-I 8524"]
[{"$nulls":6},"BGV A 2"]
["Arbeitsstellenscheinwerfer",null,null,"x","jährlich",null,"GUV-V A 2",null,null,"VDE 0702-1"]
[{"$nulls":4},"1) 5)",null,"GUV-I 8524"]
[{"$nulls":6},"BGV A 2"]
["Flutlichtstahler",null,null,"x","jährlich",null,"GUV-V A 2",null,null,"VDE 0702-1"]
[{"$nulls":4},"1) 5)",null,"GUV-I 8524"]
[{"$nulls":6},"BGV A 2"]
["Elektronenblitzleuchte",null,null,"x","jährlich",null,"GUV-V A 2",null,null,"20)"]
[null,null,null,"8)","1) ",null,"GUV-I 8524"]
[{"$nulls":6},"BGV A 2"]
["Handlautsprecher",null,null,"x","jährlich",null,"GUV-V A 2"]
[null,null,null,"8)","1) ",null,"GUV-I 8524"]
[{"$nulls":6},"BGV A 2"]
["Kabelleuchte",null,null,"x","jährlich",null,"GUV-VA 2",null,null,"VDE 0702-1"]
[{"$nulls":4},"1) 5)",null,"GUV-I 8524"]
["Leitungstrommel",null,null,"x","jährlich",null,"BGV-A 2",null,null,"VDE 0702-1"]
[{"$nulls":4},"1) 5)"]
[]
["Abzweigstück",null,null,"x","jährlich",null,"GUV-V A 2",null,null,"VDE 0702-1"]
[{"$nulls":4},"1) 5)",null,"GUV-I 8524"]
[{"$nulls":6},"BGV A 2"]
["Adapterleitungen",null,null,"x","jährlich",null,"GUV-V A 2",null,null,"VDE 0702-1"]
[{"$nulls":4},"1) 5)",null,"GUV-I 8524"]
[{"$nulls":6},"BGV A 2"]
["Warnleuchte nach StVZO",null,null,"x","jährlich",{"$nulls":4},"20)"]
[null,null,null,"8)"]
["Verkehrswarngerät",null,null,"x","jährlich"]
[null,null,null,"8)"]
["Winkerkelle (elektrisch, ",null,null,"x","jährlich"]
["beleuchtet)",null,null,"8)"]
["Handsprechfunkgerät",null,null,"x","monatlich"]
[null,null,null,"3) 8)","1) 3) 8)"]
["Ausrüstung und Geräte",null,"Prüfung bei bzw. nach",null,"Regelmäßige Prüfung",null,"Rechtsgrundlagen, Prüfgrundsätze",null,null,"Seite 8"]
[null,null,"einer Benutzung"]
["Arbeitsgerät",null,"vor einer","nach einer","Sicht und ","Belastungs-","UVV ","GUV-G 9102","Norm","Sonstige"]
[null,null,"Übung","Benutzung","Funktion","prüfung",null,"Abschnitt"]
["Spreizer",null,null,"x","jährlich","alle 3 Jahre","GUV-V C 53",16,"DIN 14751 T 1"]
[null,null,null,"1) 2) 8)","1) 2)","1) 2)",null,null,"EN 13204"]
["Schneidgerät",null,null,"x","jährlich","alle 3 Jahre","GUV-V C 53",16,"DIN 14751 T 2"]
[null,null,null,"1) 2) 8)","1) 2)","1) 2)",null,null,"EN 13204"]
["Kombigerät",null,null,"x","jährlich","alle 3 Jahre","GUV-V C 53",16,"DIN 14751 T 2"]
[null,null,null,"1) 2) 8)","1) 2)","1) 2)",null,null,"EN 13204"]
["Rettungszylinder",null,null,"x","jährlich","alle 3 Jahre","GUV-V C 53",16,"DIN 14751 T 3"]
[null,null,null,"1) 2)","1) 2)","1) 2)",null,null,"EN 13204"]
["Hydraulik-Pumpenaggregat",null,null,"x","jährlich","alle 3 Jahre","GUV-V C 53",16,"DIN 14751 T 1 - 3"]
[null,null,null,"1)","2) 5)","2) 5)",null,null,"EN 13204"]
["Hydraulische Winde",null,null,"x","jährlich","jährlich","GUV-V D 8"]
["(z.B. Büffel)",null,null,null,"2)","1) 2)","BGV D 8"]
["Hydraulischer Hebesatz ",null,null,"x","jährlich ","jährlich","GUV-V D 8",null,"DIN 14800-6"]
["(H1 + H2)",null,null,null,"2)","1) 2)","BGV D 8"]
["Luftheber 0,5 + 1,0 bar",null,null,"x","jährlich","jährlich","GUV-V C 53","4","DIN 14152"]
[null,null,null,"2)","2)","1)","GUV-V D 8"]
[{"$nulls":6},"BGV D 8"]
["Druckkissen",null,null,"x","jährlich","alle 5 Jahre","GUV-V C 53","4","DIN 14152"]
[null,null,null,"2)","2)","1) 4)"]
["Leckdichtkissen",null,null,"x","jährlich","jährlich"]
[{"$nulls":4},"3)","1)"]
["Rohrdichtkissen",null,null,"x","jährlich","jährlich"]
[{"$nulls":4},"3)","1)"]
["Mehrzweckzug",null,null,"x","jährlich",null,"GUV-V D 8",null,"DIN 14800-5"]
[{"$nulls":4},"3)",null,"BGV D 8"]
["Be- und Entlüftungsgerät",null,null,"x","jährlich"]
[{"$nulls":4},"3)"]
["Hebebaum",null,null,"x","jährlich"]
[{"$nulls":4},"3)"]
["Ausrüstung und Geräte",null,"Prüfung bei bzw. nach",null,"Regelmäßige Prüfung",null,"Rechtsgrundlagen, Prüfgrundsätze",null,null,"Seite 9"]
[null,null,"einer Benutzung"]
["Arbeitsgerät",null,"vor einer","nach einer","Sicht und ","Belastungs-","UVV ","GUV-G 9102","Norm","Sonstige"]
[null,null,"Übung","Benutzung","Funktion","prüfung",null,"Abschnitt"]
["Gulli-Dichtkissen",null,null,"x","jährlich"]
[null,null,null,"2)","3)"]
["Hubwagen",null,null,"x","jährlich","jährlich"]
[{"$nulls":4},"3)","1)"]
["Hydraulische Prüfgeräte",null,null,"x","jährlich","jährlich"]
[{"$nulls":4},"3)","1)"]
["Tragkraftspritzen",null,null,"x","halbjährlich","jährlich",null,null,"DIN 14410"]
[{"$nulls":4},"14)","8)",null,null,"prEN 14466"]
["Feuerlöschkreiselpumpen",null,null,"x","halbjährlich","jährlich",null,null,"DIN 14420"]
[{"$nulls":4},"3)","8)",null,null,"EN 1028"]
["Tauchmotorpumpen",null,null,"x","jährlich","jährlich","GUV-V A 2",null,"DIN 14425"]
[{"$nulls":5},"1) 5)","GUV-I 8524"]
[{"$nulls":6},"BGV A 2"]
["Mineralöl/Gefahrgut Umfüll- ",null,null,"x","jährlich","jährlich","GUV-V A 2",null,"DIN 14424"]
["pump. TUP 3-1,5, GUP 3-1,5",{"$nulls":4},"1) 5)","GUV-I 8524",null,"DIN 14427"]
[{"$nulls":6},"BGV A 2"]
["Fasspumpe mit Motor und ",null,null,"x","jährlich","jährlich","GUV-V A 2"]
["Pumpwerk",{"$nulls":4},"1) 5) ","GUV-I 8524"]
[{"$nulls":6},"BGV A 2"]
["Turbinentauchpumpe",null,null,"x","jährlich",null,null,null,"DIN 14426"]
[{"$nulls":4},"1) 3)"]
["Turbinenumfüllpumpe",null,null,"x","jährlich"]
[{"$nulls":4},"1) 3)"]
["Handmembranpumpe",null,null,"x","jährlich"]
[{"$nulls":4},"1) 3)"]
["Membran-Gefahrgutpumpe",null,null,"x","jährlich","jährlich","GUV-V A2"]
[{"$nulls":5},"1) 5)"]
[]
["Ausrüstung und Geräte",null,"Prüfung bei bzw. nach",null,"Regelmäßige Prüfung",null,"Rechtsgrundlagen, Prüfgrundsätze",null,null,"Seite 10"]
[null,null,"einer Benutzung"]
["Arbeitsgerät",null,"vor einer","nach einer","Sicht und ","Belastungs-","UVV ","GUV-G 9102","Norm","Sonstige"]
[null,null,"Übung","Benutzung","Funktion","prüfung",null,"Abschnitt"]
["Industriesauger",null,null,"x","jährlich",null,"GUV-V A 2",null,"EN 60335"]
[{"$nulls":4},"1) 5)",null,"GUV-I 8524"]
[{"$nulls":6},"BGV A 2"]
["Vakuumsauger (Hydrovac)",null,null,"x","jährlich"]
[{"$nulls":4},"1) 3)"]
["Exenter-Schneckenpumpe",null,null,"x","jährlich","jährlich","GUV-V A 2"]
[{"$nulls":4},"1) 3) 5)","1) 3)","GUV-I 8524"]
[{"$nulls":6},"BGV A 2"]
["Schmutzwasserpumpe",null,null,"x","jährlich",null,"GUV-V A 2"]
[{"$nulls":4},"1) 3) 5)",null,"GUV-I 8524"]
[{"$nulls":6},"BGV A 2"]
["Stromerzeuger",null,null,"x","jährlich","jährlich","GUV-V A 2",null,"DIN 14685"]
[{"$nulls":4},"1) 3) 14)","1) 5)","GUV-I 8524"]
[{"$nulls":6},"BGV A 2"]
["Motorsäge mit ",null,null,"x","jährlich",null,null,null,"EN 608"]
["Verbrennungsmotor",null,null,null,"1) 14)"]
["Motorsäge mit ",null,null,"x","jährlich",null,"GUV-V A 2"]
["Elektromotor",null,null,null,"1) 5)",null,"GUV-I 8524"]
[{"$nulls":6},"BGV A 2"]
["Trennschleifmaschine mit ",null,null,"x","jährlich",null,null,null,"EN 1454"]
["Verbrennungsmotor",null,null,null,"1) 14)"]
["Trennschleifmaschine mit ",null,null,"x","jährlich",null,"GUV-V A 2"]
["Elektromotor",null,null,null,"1) 5)",null,"GUV-I 8524"]
[{"$nulls":6},"BGV A 2"]
["Anschlagmittel/Drahtseil",null,null,"x","jährlich",null,"GUV-V 9a",17,"DIN 3051"]
[{"$nulls":6},"GUV-R 151"]
[{"$nulls":6},"BGR 151"]
["Kettengehänge, ein- und ",null,null,"x","jährlich",null,"GUV-V 9a",null,"DIN 685"]
["mehrsträngig"]
["Kunstfaserseil",null,null,"x","jährlich",null,"GUV-V 9a",17]
[{"$nulls":6},"GUV-R 152"]
[{"$nulls":6},"BGR 152"]
["Hebebänder",null,null,"x","jährlich",null,"GUV-V 9a",null,"EN 1492"]
[]
["Ausrüstung und Geräte",null,"Prüfung bei bzw. nach",null,"Regelmäßige Prüfung",null,"Rechtsgrundlagen, Prüfgrundsätze",null,null,"Seite 11"]
[null,null,"einer Benutzung"]
["Arbeitsgerät",null,"vor einer","nach einer","Sicht und ","Belastungs-","UVV ","GUV-G 9102","Norm","Sonstige"]
[null,null,"Übung","Benutzung","Funktion","prüfung",null,"Abschnitt"]
["Hebegeschirre, ",null,null,"x","jährlich",null,"GUV-V 9a"]
["mehrsträngig"]
["textile Endlosschlinge",null,null,"x","jährlich"]
[]
["Zugseil-Hebezuggerät",null,null,"x","jährlich"]
[]
["Lastaufnahmeeinrichtung",null,null,"x","jährlich",null,"GUV-V 9a"]
[]
["Handwerkzeug und",null,"vor einer","nach einer","Sicht und ","Belastungs-","UVV ","GUV-G 9102","Norm","Sonstige"]
[" Messgerät",null,"Übung","Benutzung","Funktion","prüfung",null,"Abschnitt"]
["Brennschneidgerät",null,null,"x","jährlich",null,"GUV-V D 1",null,"EN 730 "]
[{"$nulls":6},"BGV D 1",null,"DIN 14800-7"]
[{"$nulls":8},"DIN 8521"]
["Sauerstoffflasche",null,null,"x",null,"Äußere Prüfung 2 Jahre",null,null,"DIN 8546-O4","BetrSichV"]
[{"$nulls":5},"Innere Prüfung 5 J"]
[{"$nulls":5},"Festigkeitsprüfung 10 J 22)"]
["Acetylenflasche",null,null,"x",null,"Äußere Prüfung 2 Jahre",null,null,"DIN 8546-A2","BetrSichV"]
[{"$nulls":5},"Innere Prüfung 5 J"]
[{"$nulls":5},"Festigkeitsprüfung 10 J 22)"]
["Werkzeugkasten FwK",null,null,"x",{"$nulls":4},"DIN 14881"]
[]
["Werkzeugkasten E",null,null,"x","jährlich",null,null,null,"DIN 14885"]
[]
["Werkzeugkasten ",null,null,"x","jährlich"]
["(3 tlg. + 5 tlg.)"]
["Handwerkzeug und",null,"vor einer","nach einer","Sicht und ","Belastungs-","UVV ","GUV-G 9102","Norm","Sonstige"]
[" Messgerät",null,"Übung","Benutzung","Funktion","prüfung",null,"Abschnitt"]
["Filmdosimeter",null,"Austausch der Filmplakette erfolgt durch die amtliche Auswertestelle"]
[]
["Dosisleistungsmeßgerät",null,null,"x","halbjährlich"]
[]
["Ausrüstung und Geräte",null,"Prüfung bei bzw. nach",null,"Regelmäßige Prüfung",null,"Rechtsgrundlagen, Prüfgrundsätze",null,null,"Seite 12"]
[null,null,"einer Benutzung"]
["Handwerkzeug und",null,"vor einer","nach einer","Sicht und ","Belastungs-","UVV ","GUV-G 9102","Norm","Sonstige"]
[" Messgerät",null,"Übung","Benutzung","Funktion","prüfung",null,"Abschnitt"]
["Dosisleistungswarngerät",null,null,"x","halbjährlich"]
[]
["Dosiswarngerät",null,null,"x","halbjährlich"]
[]
["Kontaminations-",null,null,"x","halbjährlich"]
["nachweisgerät"]
["Ex-, Ex-/Ox-Messgerät",null,null,"x","1)",null,null,null,"EN 50057"]
[{"$nulls":8},"EN 50104"]
["Sensormessgerät",null,null,"x","1)"]
[]
["Infrarotspektrometer",null,null,"x","1)"]
[]
["Handwerkzeug und",null,"vor einer","nach einer","Sicht und ","Belastungs-","UVV ","GUV-G 9102","Norm","Sonstige"]
[" Messgerät",null,"Übung","Benutzung","Funktion","prüfung",null,"Abschnitt"]
["Photoionisationsdetektor",null,null,"x","1)"]
[]
["Photometer",null,null,"x","1)"]
[]
["Leitfähigkeitsmessgerät",null,null,"x","vierteljährlich"]
[]
["pH-Messgerät",null,null,"x","vierteljährlich"]
[]
["Prüfröhrchen",null,null,"x",null,"Verbrauchszeit der Röhrchen beachten (in der Regel 2 Jahre)"]
[]
["Pumpe für Prüfröhrchen",null,null,"x","1)"]
[]
["pH-Papier",null,null,"x","1)"]
[]
["Öltestpapier",null,null,"x","1)"]
[]
["Wasseranalyseset",null,null,"x","1)"]
[]
["Heustockmesssonde",null,null,"x","1)"]
[]
["Ausrüstung und Geräte",null,"Prüfung bei bzw. nach",null,"Regelmäßige Prüfung",null,"Rechtsgrundlagen, Prüfgrundsätze",null,null,"Seite 13"]
[null,null,"einer Benutzung"]
["Sondergerät",null,"vor einer","nach einer","Sicht und ","Belastungs-","UVV ","GUV-G 9102","Norm","Sonstige"]
[null,null,"Übung","Benutzung","Funktion","prüfung",null,"Abschnitt"]
["Kraftstoffkanister aus PE",null,null,null,"monatlich","Kraftstoffkanister aus Polyethylen sind 6 Jahre  nach Herstellungsdatum auszumustern "]
[{"$nulls":4},"3)","(GGVS). Datum auf dem Kanister."]
["Doppelkanister für ",null,null,null,"monatlich"]
["Kettensägen aus PE",null,null,null,"3)"]
["Ausrüstung und Geräte",null,"Prüfung bei bzw. nach",null,"Regelmäßige Prüfung",null,"Rechtsgrundlagen, Prüfgrundsätze",null,null,"Seite 12"]
[null,null,"einer Benutzung"]
["Geräte im Fw-Haus",null,"vor einer","nach einer","Sicht und ","Belastungs-","UVV ","GUV-G 9102","Norm","Sonstige"]
[null,null,"Übung","Benutzung","Funktion","prüfung",null,"Abschnitt"]
["Tore, kraftbetätigt",null,null,"jährlich",null,null,"GUV-R 1/494"]
[]
["elektrische Anlagen,",null,null,"vierjährig",null,null,"GUV-V A 2"]
[{"$nulls":6},"GUV-I 8524"]
[{"$nulls":6},"BGV-A 2"]
["Flüssigkeitsstrahler",null,null,"jährlich",null,null,"GUV-V D 15"]
[{"$nulls":6},"BGV D 15"]
["Feuerwehrfahrzeuge",null,"x","x","jährlich",null,"GUV-V D 29",null,14502,"STVZO"]
[{"$nulls":6},"GUV-R 157",null,"EN 1846","GUV 15.6"]
[{"$nulls":6},"BGV D 29",null,null,"BGG 915"]
[{"$nulls":6},"BGR 157",null,null,"und 916"]
["Flurförderzeuge",null,"x","x",null,null,"BGV D 27"]
[{"$nulls":4},"jährlich 2)"]
["Winden",null,"x","x","jährlich 2)",null,"BGV D 8"]
["Hebebühnen ",null,null,null,"jährlich 2)",null,"VBG 14"]
[{"$nulls":6},"BGI 689"]
["Krane",null,"x","x","jährlich 2)","alle 4 Jahre 4)","BGV D 8"]
[{"$nulls":6},"BGV D 6"]
[{"$nulls":6},"BGI 610"]
[{"$nulls":6},"BGG 905"]
["Druckbehälter",null,"Prüfung gemäß Betriebssicherheitsverordnung",null,null,"siehe Bemerkungen hier"]
[]
["Bedeutung der in der Geräteprüftabelle genannten Fußnoten"]
[null,"1)","Gerät ist nach Herstellervorschriften zu prüfen"]
[null,"2)","Prüfung durch einen Sachkundigen"]
[null,"3)","Empfehlung zur Sicherstellung der Schutzfunktion und Funktionsfähigkeit"]
[null,"4)","Prüfung durch Sachverständigen und / oder Hersteller"]
[null,"5)","Prüfung nicht ortsfester Elektrogeräte erfolgt durch eine Fachkraft"]
[null,null,"oder einer in der Elektrotechnik unterwiesenen Person"]
[null,"6)","Hier sind in jährlichem Abstand Vollzähligkeit und Gesamtzustand zu prüfen.",{"$nulls":4},"Um die Aktualität der Liste gewährleisten"]
[]
[]
[]
[null,null,"(z.B. Nähte, Knöpfe, Hosenträger, Reißverschluss)",{"$nulls":4},"zu können, wird gebeten, Hinweise auf"]
[null,"7)","Unversehrtheit der Verschlüsse",{"$nulls":4},"fehlerhafte Eintragungen, Veränderungs- "]
[null,"8)","Akku- und Batteriegeräte auf Ladezustand überprüfen",{"$nulls":4},"und Ergänzungswünsche an folgende"]
[null,"9)","Medizingeräteverordnung",{"$nulls":4},"e-mail-Adresse zu senden:"]
[null,"10)","Prüfung der Gebrauchfähigkeit, Sauberkeit, Desinfektion",{"$nulls":4},"Fleck@fws.bwl.de"]
[null,"11)","Prüfung auf weitere Verwendbarkeit des Gerätes",{"$nulls":4},"Stand: 24.05.04"]
[null,"12)","Prüfung der Sauerstoffflasche je nach Größe"]
[null,"13)","Ein durch Absturz beanspruchter Gurt ist sofort zu prüfen"]
[null,"14)","Besondere Hinweise der Motorhersteller beachten"]
[null,"15)","Es wird empfohlen, mindestens einmal jährlich eine Übung mit dem Gerät durchzuführen (Handhabung) "]
[null,"16)","Herstellungsrichtlinien der Länder"]
[null,"17)","Prüffristen siehe GUV-G 9102"]
[null,"18)","Bei luftdich verpackten Vollmasken oder Masken-Helm-Kombinationen ist die Sicht- und Funktionsprüfung alle 2 Jahre ausreichend,"]
[null,null,"ggf. halbjährlich Stichproben durchführern"]
[null,"19)","Wenn Behälter nachgefüllt wird"]
[null,"20)","Prüfzeichen und Zulassung des BMVBW muss auf dem Gerät vorhanden sein."]
[null,"21)","Prüfung auf Wasserhalbzeit empfohlen"]
[null,"22)","Maximaler Zeitraum;  Das Prüfintervall ist ggf. im Einzelfall nach der Betriebssicherheitsverordnung mit der Prüfstelle zu vereinbaren"]
[null,"23)","Broschüre \"Persönliche Schutzausrüstung\" über den Link: www.uk_bw.de/download/schutz_feuerwehr.pdf"]
[]
["Anhang 1"]
[]
["Wartungsarbeiten und -fristen für Vollmasken von Pressluftatmern"]
[]
[]
["Art der Arbeiten",null,"Längstzulässige Fristen "]
[]
[null,null,"Vor ","Nach","Halb-","Zwei ","Vier","Sechs"]
[null,null,"Gebrauch","Gebrauch","jährlich","Jahre","Jahre","Jahre"]
[]
["Reinigung und Desinfektion ",null,null,"x",null,"x"]
[]
["Sicht-, Funktions- und Dichtprüfung",null,null,"x","x"]
[]
["Wechsel der Ausatemventilscheibe",{"$nulls":5},"x"]
[]
["Wechsel der Sprechmembrane",{"$nulls":6},"x"]
[]
["Kontrolle durch den Geräteträger",null,"x"]
[]
["Quelle: vfdb-Richtlinie 0804 Stand: 04/2002"]
[]
[]
[]
[]
["Anhang 2"]
[]
["Wartungsarbeiten und -fristen für Pressluftatmer (o. Atemanschluss)"]
[]
[]
["Gerät",null,"Art der Arbeiten",null,"Längstzulässige Fristen"]
[]
[{"$nulls":4},"Vor ","Nach ","Halb-","Zwei ","Vier","Sechs"]
[{"$nulls":4},"Gebrauch","Gebrauch","jährlich","Jahre","Jahre","Jahre"]
[]
["Pressluftatmer, komplett",null,"Reinigung",null,null,"x","x"]
[]
[null,null,"Sicht-, Funktions-",null,null,"x","x"]
[null,null,"und Dichtprüfung"]
[]
[null,null,"Kontrolle durch",null,"x"]
[null,null,"den Gräteträger"]
[]
["Lungenautomat",null,"Reinigung und",null,null,"x",null,"x"]
[null,null,"Desinfektion"]
[]
[null,null,"Wechsel der ",{"$nulls":4},"x","x"]
[null,null,"Membran"]
[]
[null,null,"Sicht-, Funktions-",null,null,"x","x"]
[null,null,"und Dichtprüfung"]
[]
["Lungenautomat ein-",null,"Grundüberholung",{"$nulls":6},"x"]
["schließlich Schlauch"]
[]
["Pressluftatmer mit",null,"Grundüberholung",{"$nulls":6},"x"]
["Tragevorrichtung,"]
["ohne Lungenautomat"]
["ohne Atemluftflasche"]
[]
["Quelle: vfdb-Richtlinie 0804 Stand:04/2002"]