{"text_format":"2","workbook":"xls","n_sheets":9,"sheets":["A_Gruppe1","A_Gruppe2","A_Gruppe3","A_Gruppe4","A_Gruppe5","A_Gruppe6","A_Gruppe7","A_Gruppe8","A_Gruppe9"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":7,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"A_Gruppe1","index":0,"n_rows":61,"n_cols":10,"rows_kept":61,"cut":false,"hidden":false,"merged":[[5,0,5,3]],"flags":["formulas_cached_only"]}
["Die Gruppe 1 unterteilt sich in folgende Untergruppen:"]
[1,1,null,null,"Schutzkleidung"]
[1,2,null,null,"Atemschutzgerät"]
[1,3,null,null,"Tauchergerät"]
[]
["Nr.",null,null,null,"Benennung nach Norm","nach DIN","Masse","weitere Benennungen","Anzahl","Masse"]
[1,1,1,1,"Feuerwehrüberjacke","EN 469",2,"Brandschutzjacke",null,0]
[1,1,2,1,"Warnkleidung W1 (Weste)","EN 471",0.5,"",null,0]
[1,1,3,1,"Wathose mit Stiefel S5","EN 345",4.5,"",null,0]
[1,1,4,1,"Schutzschuhe S 5 (Paar) (Gummistiefel)","EN 345",2.5,"",null,0]
[1,1,5,1,"Schutzschuhe S 5 (Paar) mit Hochschaft","EN 345",3.2,"Kanalarbeiterstiefel",null,0]
[1,1,6,1,"Arbeitsschutzhandschuhe nach UVV Feuerwehr (Paar)","EN 420 K1",0.3,"",null,0]
[1,1,6,2,"Feuerwehrhandschuh","EN 659",0.3,"",null,0]
[1,1,6,3,"Chemikalienschutzhandschuhe mit Stulpen Öl/Säure","EN 374",0.3,"",null,0]
[1,1,7,1,"Schutzbrille mit Klarscheiben","58210",0.2,"",null,0]
[1,1,7,2,"Augenschutzbrille für Feuerwehrhelm","EN 166",0.2,"",null,0]
[1,1,7,3,"Schweißerschutzbrille","4644",0.05,"",null,0]
[1,1,7,4,"Vollsichtschutzbrille","EN 166",0.2,"",null,0]
[1,1,8,1,"Gesichtsschutz zum Fw-Helm","EN 166",0.3,"Klappvisier",null,0]
[1,1,9,1,"Einwegschutzanzug Schutzklasse 3-5","EN 368",0.6,"",null,0]
[1,1,10,1,"Hitzeschutzkleidung Form I","1486",1.7,"",null,0]
[1,1,10,2,"Hitzeschutzkleidung Form II","1486",6,"",null,0]
[1,1,10,3,"Hitzeschutzkleidung Form III","1486",12.5,"",null,0]
[1,1,11,1,"Chemikalienschutzanzug Form I","EN 943",2.5,"",null,0]
[1,1,11,2,"Chemikalienschutzanzug Form II","EN 943",7.6,"",null,0]
[1,1,11,3,"Chemikalienschutzanzug Form III","EN 943",8,"",null,0]
[1,1,12,1,"Kontaminationsschutzkleidung Form I","",1,"Haube",null,0]
[1,1,12,2,"Kontaminationsschutzkleidung Form II","",2,"",null,0]
[1,1,12,3,"Kontaminationsschutzkleidung Form III","",8,"identisch CSA",null,0]
[1,1,13,1,"Rettungsweste (Schwimmweste)","EN 395",0.8,"",null,0]
[1,1,13,2,"Rettungsfeuerwehrweste (zur Verwendung mit PA)","EN 399",1.2,"Schwimmweste",null,0]
[1,1,14,1,"Schnittschutzhose Form C","EN 381-5",1.5,"Latzhose für Waldarbeiter",null,0]
[1,1,14,2,"Schnittschutzjacke","EN 381-5",1,"",null,0]
[1,1,15,1,"Schutzhelm für Kettensägenführer","EN 352-3",0.6,"",null,0]
[1,1,15,2,"Feuerwehrhelm","EN 443",1.2,"",null,0]
[1,1,15,3,"Schutzhelm für Höhenretter","EN 397",0.5,"",null,0]
[1,1,16,1,"Gehörschutzstöpsel,VPE","",0.5,"",null,0]
[1,1,16,2,"Gehörschutzbügel","EN 352",0.2,"",null,0]
[1,2,1,1,"Atemanschluß (Vollmaske)","EN 148 / 136",0.6,"",null,0]
[1,2,2,1,"Tragebüchse für Atemanschluß","",0.7,"",null,0]
[1,2,3,1,"Umluftunabhängiges Atemschutzgerät, ohne Atemanschluss","EN 137",17.5,"",null,0]
[1,2,4,1,"Druckluftflasche gefüllt, Stahl, 2 l / 300 bar",3171,4.8,"",null,0]
[1,2,4,2,"Druckluftflasche gefüllt, Stahl, 4 l / 200 bar  ","EN 12245",6.1,"",null,0]
[1,2,4,3,"Druckluftflasche gefüllt, Stahl, 6 l / 300 bar  ","EN 12245",11.5,"",null,0]
[1,2,5,1,"Druckluftflasche gefüllt, CFK, 2 l / 300 bar","EN 12245",2.8,"",null,0]
[1,2,5,2,"Druckluftflasche gefüllt, CFK, 3 l / 300 bar","EN 12245",4,"",null,0]
[1,2,5,3,"Druckluftflasche gefüllt, CFK, 6 l / 300 bar  ","EN 12245",6.5,"",null,0]
[1,2,5,4,"Druckluftflasche gefüllt, CFK, 6,8 l / 300 bar  ","EN 12245",7.3,"",null,0]
[1,2,6,1,"Regenerationsgerät (2 Stunden)","EN 145",13.5,"",null,0]
[1,2,6,2,"Regenerationsgerät (4 Stunden)","EN 145",18,"",null,0]
[1,2,7,1,"Mehrbereichsfilter A2B2E2K2P3","EN 148",0.4,"Kombinationsfilter",null,0]
[1,2,8,1,"Filtergerät mit Haube zur Selbstrettung (Fluchthaube)","EN 403",0.7,"Brandfluchthaube",null,0]
[1,2,9,1,"Feinstaubmaske FFP 3 S","EN 149",0.01,"",null,0]
[1,3,1,1,"Taucherschutzanzug ","",4,"",null,0]
[1,3,2,1,"Feuerwehrtauchgerät (nach VFDB 0803)","EN 250",20,"",null,0]
[1,3,3,1,"Reserveflaschen für Feuerwehrtauchgerät","",12,"",null,0]
[1,3,4,1,"Gewichtsgürtel","",0,"",null,0]
[1,3,5,1,"Tauchermesser","",0.6,"",null,0]
[1,3,6,1,"Führungsleine / Sicherheitsleine 50 m","EN 892-1",0,"",null,0]
[]
[{"$nulls":7},"Gesamtmasse der ausgewählten Ausrüstung:",null,0]

{"sheet":"A_Gruppe2","index":1,"n_rows":54,"n_cols":10,"rows_kept":54,"cut":false,"hidden":false,"merged":[[5,0,5,3]],"flags":["formulas_cached_only"]}
["Die Gruppe 2 unterteilt sich in folgende Untergruppen:"]
[2,1,null,null,"Sonstige Löschgeräte"]
[2,2,null,null,"Feuerlöscher"]
[2,3,null,null,"Schaumausrüstung"]
[]
["Nr.",null,null,null,"Benennung nach Norm","nach DIN","Masse","weitere Benennungen","Anzahl","Masse"]
[2,1,1,1,"Feuerpatsche mit Stiel; 2,0 m lang","",2,"Waldbrandpatsche",null,0]
[2,1,2,1,"Löschdecke in wiederverwendbarer Schutzhülle","14155",3,"",null,0]
[2,2,1,1,"Kübelspritze A10, gefüllt","14405",20,"",null,0]
[2,2,2,1,"Wasserlöscher W 6l H - 30°   A","EN 3",12.9,"",null,0]
[2,2,2,2,"Wasserlöscher W 6l L 0- 60°  A","EN 3",10.7,"",null,0]
[2,2,2,3,"Wasserlöscher W 9l H - 0°    A","EN 3",16.4,"",null,0]
[2,2,2,4,"Wasserlöscher W 9l H - 30°  A","EN 3",16.9,"",null,0]
[2,2,2,5,"Wasserlöscher W 9l L 0- 60°  A","EN 3",14.9,"",null,0]
[2,2,3,6,"Schaumlöscher S 9 H 0 - 60° AB   (AFFF)","EN 3",15.9,null,null,0]
[2,2,3,1,"Schaumlöscher S 6 L   +     AB","EN 3",10.9,null,null,0]
[2,2,3,2,"Schaumlöscher S 6 L  - 30° AB","EN 3",10.7,null,null,0]
[2,2,3,3,"Schaumlöscher S 6 H 0 - 60° AB   (AFFF)","EN 3",12,null,null,0]
[2,2,3,4,"Schaumlöscher S 9 L  +      AB","EN 3",15,null,null,0]
[2,2,3,5,"Schaumlöscher S 9 L  - 30° AB","EN 3",14.8,null,null,0]
[2,2,4,1,"Pulverlöscher L 1 kg           ABC ","EN 3",1.5,null,null,0]
[2,2,4,2,"Pulverlöscher L 1,3 kg        ABC","EN 3",2.4,null,null,0]
[2,2,4,3,"Pulverlöscher L 2 kg           ABC ","EN 3",3.4,null,null,0]
[2,2,4,4,"Pulverlöscher L 4 kg           ABC ","EN 3",7,null,null,0]
[2,2,4,5,"Pulverlöscher L 6 kg           ABC ","EN 3",9.9,null,null,0]
[2,2,4,6,"Pulverlöscher L 9 kg           ABC ","EN 3",13.6,null,null,0]
[2,2,4,7,"Pulverlöscher L 12 kg          ABC ","EN 3",17.5,null,null,0]
[2,2,4,10,"Pulverlöscher H 6 kg           ABC ","EN 3",11.3,null,null,0]
[2,2,4,11,"Pulverlöscher H 9 kg           ABC ","EN 3",15.3,null,null,0]
[2,2,4,12,"Pulverlöscher H 12 kg         ABC ","EN 3",19,null,null,0]
[2,2,4,15,"Pulverlöscher H 6 kg           BC ","EN 3",11,null,null,0]
[2,2,4,16,"Pulverlöscher H 12 kg         BC ","EN 3",20,null,null,0]
[2,2,4,20,"Metallbrandlöscher H 12 kg D","EN 3",20,null,null,0]
[2,2,4,25,"Pulverlöscher H 50 kg         ABC","EN1866",100,null,null,0]
[2,2,5,1,"Kohlendioxid Löscher K 2    B","EN 3",7.5,null,null,0]
[2,2,5,2,"Kohlendioxid Löscher K 5    B","EN 3",15.4,null,null,0]
[2,2,5,3,"Kohlendioxid Löscher K 6    B",null,16,"",null,0]
[2,2,5,4,"Kohlendioxid Löscher K 10  B","Anl. EN 3",53,"",null,0]
[2,2,5,5,"Kohlendioxid Löscher K 20  B","Anl. EN 3",74,"",null,0]
[2,2,5,6,"Kohlendioxid Löscher K 30  B","Anl. EN 3",94,"",null,0]
[2,2,5,7,"Kohlendioxid Löscher K 60  B","Anl. EN 3",173,"",null,0]
[2,2,6,1,"Fettbrandlöscher F 6l H - 0° AF","EN 3",12.5,null,null,0]
[2,2,6,2,"Fettbrandlöscher F 9l H - 0° AF","EN 3",16.7,null,null,0]
[2,2,7,1,"Löschgerät, tragbar, befüllbar ca. 10 l ","Anl. EN 3",25,"Hochdrucklöschgeräte",null,0]
[2,3,1,1,"Zumischer Z2R","14384",4.5,"",null,0]
[2,3,1,2,"Zumischer Z4R","14384",5,"",null,0]
[2,3,1,3,"Zumischer Z8R","14384",6.5,"",null,0]
[2,3,1,5,"Zumischer LZ2R","14384",2.2,"",null,0]
[2,3,1,6,"Zumischer LZ4R","14384",2.6,"",null,0]
[2,3,1,7,"Zumischer LZ8R","14384",2.7,"",null,0]
[2,3,2,1,"Turbozumischer TR4","",12,"",null,0]
[2,3,3,1,"Schaummittelbehälter 20 l ","14452",25,"Schaummittelkanister",null,0]
[]
[{"$nulls":7},"Gesamtmasse der ausgewählten Ausrüstung:",null,0]

{"sheet":"A_Gruppe3","index":2,"n_rows":134,"n_cols":10,"rows_kept":134,"cut":false,"hidden":false,"merged":[[9,0,9,3]],"flags":["formulas_cached_only"]}
["Die Gruppe 3 unterteilt sich in folgende Untergruppen:"]
[3,1,null,null,"Druckschläuche"]
[3,2,null,null,"Saugschläuche"]
[3,3,null,null,"Armaturen"]
[3,4,null,null,"Strahlrohre"]
[3,5,null,null,"Schaumstrahlrohre, Sondergeräte zur Wasserabgabe"]
[3,6,null,null,"Zubehör"]
[3,7,null,null,"Schläuche, Armaturen und Zubehör zur Größe \"F\""]
[]
["Nr.",null,null,null,"Benennung nach Norm","nach DIN","Masse","weitere Benennungen","Anzahl","Masse"]
[3,1,1,1,"Druckschlauch A 110-5-K",14811,8.8,"",null,0]
[3,1,1,2,"Druckschlauch A 110-20 -K",14811,26.8,"",null,0]
[3,1,2,1,"Druckschlauch B 75-5-K",14811,5,"",null,0]
[3,1,2,2,"Druckschlauch B 75-20-K",14811,13.12,"",null,0]
[3,1,2,3,"Druckschlauch B 75-35-K",14811,27.8,"",null,0]
[3,1,3,1,"Druckschlauch C 52-15-K",14811,7,"",null,0]
[3,1,4,1,"Druckschlauch C 42-15-K",14811,5.49,"",null,0]
[3,1,4,2,"Druckschlauch C 42-30-K",14811,11.4,"",null,0]
[3,1,5,1,"Druckschlauch D 25-5-K",14811,1.4,"",null,0]
[3,1,5,2,"Druckschlauch D 25-15-K",14811,3.8,"",null,0]
[3,1,6,1,"Druckschlauch C 52-15-K mineralölbeständig","",9,"Ölwehr-Druckschläuche",null,0]
[3,1,7,1,"Druckschlauch C 42-15-K für Pulver",null,7.6,"",null,0]
[3,1,7,2,"Druckschlauch C 42-30-K für Pulver","",15,"",null,0]
[3,1,8,1,"Feuerlöschschlauch 50 m, DN 25","EN 1947",23,"Schnellangriffschlauch",null,0]
[3,1,8,2,"Feuerlöschschlauch 30 m, DN 32","EN 1947",16,"Schnellangriffschlauch",null,0]
[3,2,1,1,"Feuerlöschschlauch A 110-1500-K","14557",14,"Saugschlauch",null,0]
[3,2,1,2,"Feuerlöschschlauch A 110-2400-K",14557,19,"Saugschlauch",null,0]
[3,2,2,1,"Feuerlöschschlauch B-1500-K",14557,7.6,"Saugschlauch",null,0]
[3,2,3,1,"Feuerlöschschlauch C-1500-K",14557,4.6,"Saugschlauch",null,0]
[3,2,4,1,"Ansaugschlauch D 1500",14819,0.8,"",null,0]
[3,2,4,2,"Ansaugschlauch D 3000",14819,1.5,"",null,0]
[3,2,5,1,"Saugschlauch C-1500-K mineralölbeständig","",6,"",null,0]
[3,2,6,1,"Saugschlauch, D = 38 mm, 1,5 m lang","",3.9,"",null,0]
[3,3,1,1,"Saugkorb A","14362",6,"",null,0]
[3,3,1,2,"Kellersaugkorb A","",4.4,"",null,0]
[3,3,2,1,"Saugkorb B","14362",3.5,"",null,0]
[3,3,3,1,"Saugkorb C","14362",1,"",null,0]
[3,3,3,2,"Saugkorb C ölbeständig","14362",3.3,"",null,0]
[3,3,4,1,"Saugschutzkorb A (Draht)","",1.3,"",null,0]
[3,3,4,2,"Saugschutzkorb B (Draht)","",1,"",null,0]
[3,3,4,3,"Saugschutzkorb C (Draht)","",0.7,"",null,0]
[3,3,5,1,"Standrohr 2B","14375",7.2,"",null,0]
[3,3,5,2,"Schlüssel C (Unterflurhydrant)","3223",5.6,"",null,0]
[3,3,5,3,"Standrohr 2B (Ausf. Württemberg)","",8.8,"",null,0]
[3,3,5,4,"Schlüssel C (Unterflurhydrant-Württemberg)","3223-W",10,"",null,0]
[3,3,5,5,"Standrohrhalter (Württemberg)",null,4,"",null,0]
[3,6,5,6,"Schlüssel B (Überflurhydrant)","3223",2.2,"",null,0]
[3,3,6,1,"Sammelstück A-2B","14355",3.6,"",null,0]
[3,3,6,2,"Sammelstück A-3B","",7.1,"",null,0]
[3,3,6,3,"Sammelstück A-4B","",9.3,"",null,0]
[3,3,7,1,"Verteiler B-CBC (Niederschraubventil)","14345",6,"",null,0]
[3,3,7,2,"Verteiler B-CBC (Kugelhahn)","14345",7,"",null,0]
[3,3,8,1,"Verteiler BB-CBC (Kugelhahn)","",8.1,"",null,0]
[3,3,9,1,"Verteiler C-DCD (Niederschraubventil)","14345",3,"",null,0]
[3,3,9,2,"Verteiler C-DCD (Kugelhahn)","14345",2.2,"",null,0]
[3,3,10,1,"Übergangsstück A-B","14343",1.5,"",null,0]
[3,3,10,2,"Übergangsstück B-C","14342",0.7,"",null,0]
[3,3,10,3,"Übergangsstück C-D","14341",0.4,"",null,0]
[3,3,11,1,"Druckbegrenzungsventil B","14380",6,"",null,0]
[3,3,12,1,"Wasserstrahlpumpe C-B","14422",8,"",null,0]
[3,4,1,1,"Strahlrohr BM","14365-1",2.7,"",null,0]
[3,4,1,2,"Stützkrümmer SK","14368",2,"",null,0]
[3,4,1,3,"Strahlrohr B >400 l/min mit Stützkrümmer (Hohlstrahlrohr)","14367",5.5,"",null,0]
[3,4,1,4,"Strahlrohr B für Druckluftschaum","",2.5,"",null,0]
[3,4,2,1,"Strahlrohr CM",14365,1.8,"",null,0]
[3,4,2,2,"Strahlrohr C <400 l/min (Hohlstrahlrohr)","14367",3.5,"",null,0]
[3,4,2,3,"Strahlrohr C (Pistole)","",3.5,"",null,0]
[3,4,2,4,"Strahlrohr C für Druckluftschaum","",2.2,"",null,0]
[3,4,2,5,"Strahlrohr C für Löschpulver","",3.5,"",null,0]
[3,4,2,6,"Strahlrohr C für Wassernebel","",5,"Zerstäuberstrahlrohr",null,0]
[3,4,3,1,"Strahlrohr DM",14365,1,"",null,0]
[3,4,3,2,"Strahlrohr D <150 l/min (Hohlstrahlrohr)","",2.5,"",null,0]
[3,4,4,1,"Löschlanze D - Set","",12.5,"Fognail",null,0]
[3,4,4,2,"Löschlanze C","",7,"",null,0]
[3,5,1,1,"Schaumstrahlrohr S2","14366",2.3,"",null,0]
[3,5,1,2,"Schaumstrahlrohr S4","14366",3.5,"",null,0]
[3,5,1,3,"Schaumstrahlrohr S8","14366",7,"",null,0]
[3,5,2,1,"Schaumstrahlrohr M2 / M2W","14366",4,"",null,0]
[3,5,2,2,"Schaumstrahlrohr M4 / M4W","14366",4.5,"",null,0]
[3,5,2,3,"Schaumstrahlrohr M8 / M8W","14366",7,"",null,0]
[3,5,3,1,"Kombinationsschaumrohr M2/S2-C","14366",5.5,"",null,0]
[3,5,3,2,"Kombinationsschaumrohr M4/S4-B","14366",8,"",null,0]
[3,5,4,1,"Schaumaufsatz für Hohlstrahlrohr C","",1,"",null,0]
[3,5,4,2,"Schaumaufsatz für Hohlstrahlrohr B","",1.5,"",null,0]
[3,5,5,1,"Mittelschaumpistole","",2,"",null,0]
[3,5,6,1,"Hydroschild C","",2.5,"",null,0]
[3,5,6,2,"Hydroschild B","",4.5,"",null,0]
[3,5,7,1,"Wasserwerfer, tragbar <2000 l/min (leichte Ausführung)","",15,"",null,0]
[3,5,7,2,"Wasserwerfer, tragbar <2000 l/min (schwere Ausführung)","",25,"",null,0]
[3,5,7,3,"Wasserwerfer, tragbar >2000 l/min","",35,"",null,0]
[3,6,1,1,"Mehrzweckleine 20 m","14920",1.7,"Arbeitsleine, Halteleine, Ventilleine",null,0]
[3,6,2,1,"Rollschlauchriemen B-C","14829",0.1,null,null,0]
[3,6,3,1,"Seilschlauchhalter 1600-H od. KF","14828",0.15,"",null,0]
[3,6,3,2,"Gurtschlauchhalter 350","14828",0.7,"",null,0]
[3,6,4,1,"Schlauchbrücke 2B-Holz","14820-1",12,"",null,0]
[3,6,4,2,"Schlauchbrücke 2B-Aluminium","14820-2",18,"",null,0]
[3,6,4,3,"Schlauchbrücke 2B-Kunststoff","",12,"",null,0]
[3,6,4,4,"Rohr-Schlauchüberführung 2B","14821",90,"",null,0]
[3,6,5,1,"Schlauchhaspel tragbar","14825",13,"",null,0]
[3,6,5,2,"Schlauchhaspel fahrbar (Zweipersonen-Schlauchhaspel)","14826-1",95,"",null,0]
[3,6,5,3,"Fahrbare Einpersonen-Schlauchhaspel","14826-2",75,"",null,0]
[3,6,6,1,"Schlauchtragekorb B STK-B","12827-1",4.5,"",null,0]
[3,6,6,2,"Schlauchtragekorb C STK-C","14827-1",4,"",null,0]
[3,6,6,3,"Schlauchtragekorb D STK-D","14827-1",3,"",null,0]
[3,6,6,4,"Schlauchtragekorb für den Schnellangriff STK-S","14827-2",7,"",null,0]
[3,6,7,1,"Eimer 10 l, Segeltuch","",0.5,"",null,0]
[3,6,7,2,"Eimer 10 l, Kunststoff","",0.4,"",null,0]
[3,6,7,3,"Eimer 10 l, Stahl verzinkt","",1.4,"",null,0]
[3,6,8,1,"Kupplungsschlüssel ABC","14822-2",0.7,"",null,0]
[3,6,8,2,"Kupplungsschlüssel BC","14822-1",0.3,"",null,0]
[3,6,8,3,"Kupplungsschlüssel BC-nicht funkenreißend","14822-1",0.5,"",null,0]
[3,6,9,1,"Paar Schachthaken mit Kette","",0.6,"",null,0]
[3,6,9,2,"Schachtdeckelheber mit Griff","",1.2,"",null,0]
[3,6,10,1,"Hebelschlauchbinde C","14108",0.3,"",null,0]
[3,6,10,2,"Hebelschlauchbinde B","14108",0.6,"",null,0]
[3,6,10,3,"Universalschlauchbinde","",0.1,"",null,0]
[3,7,11,1,"Kreuzverteiler F mit 2 Blindkupplungen",null,20,null,null,0]
[3,7,11,2,"Verteiler F-FF",null,12.5,"F- Y Teilstück",null,0]
[3,7,11,3,"Verteiler F-BBBBB",null,18,"F- Mehrfach Teilstück 1xFauf 5xB",null,0]
[3,7,11,4,"Absperrschieber F",null,10.5,null,null,0]
[3,7,11,5,"Rückschlagklappe F",null,9,null,null,0]
[3,7,11,6,"Übergangstück F-A",null,4,null,null,0]
[3,7,11,7,"Sammelstück F-2A",null,12,null,null,0]
[3,7,11,8,"Festkupplung F 150DS",null,2,null,null,0]
[3,7,11,9,"Blindkupplung F",null,2.5,null,null,0]
[3,7,11,10,"Übergangstück F-A125",null,4.5,null,null,0]
[3,7,12,1,"Kupplungsschlüssel F",null,1.2,null,null,0]
[3,7,13,1,"Druckschlauch F-5-K",14811,16,null,null,0]
[3,7,13,2,"Druckschlauch F-10-K",14811,24,null,null,0]
[3,7,13,3,"Druckschlauch F-20-K",14811,40,null,null,0]
[3,7,13,4,"Druckschlauch F-40-K",14811,71,null,null,0]
[3,7,13,5,"Druckschlauch F-50-K",14811,87,null,null,0]
[]
[{"$nulls":7},"Gesamtmasse der ausgewählten Ausrüstung:",null,0]

{"sheet":"A_Gruppe4","index":3,"n_rows":42,"n_cols":10,"rows_kept":42,"cut":false,"hidden":false,"merged":[[8,0,8,3]],"flags":["formulas_cached_only"]}
["Die Gruppe 4 unterteilt sich in folgende Untergruppen:"]
[4,1,null,null,"Tragbare Leitern"]
[4,2,null,null,"Sprungrettungsgerät"]
[4,3,null,null,"Wasserrettungsgerät"]
[4,4,null,null,"Tierrettungsgerät"]
[4,5,null,null,"PSA gegen Absturz"]
[4,6,null,null,"Sonstiges Rettungsgerät"]
[]
["Nr.",null,null,null,"Benennung nach Norm","nach DIN","Masse","weitere Benennungen","Anzahl","Masse"]
[4,1,1,1,"Schiebleiter, 3-teilig, SL3-H","EN 1147",100,"",null,0]
[4,1,1,2,"Schiebleiter, 3-teilig, SL3-LM","EN 1147",80,"",null,0]
[4,1,2,1,"Steckleiter, 4-teilig, 4-H","EN 1147",50,"",null,0]
[4,1,2,2,"Steckleiterteil-H","EN 1147",12.5,"",null,0]
[4,1,2,3,"Einsteckteil HE","EN 1147",4,"",null,0]
[4,1,2,4,"Steckleiter, 4-teilig, 4-LM","EN 1147",40,"",null,0]
[4,1,2,5,"Steckleiterteil-LM","EN 1147",10,"",null,0]
[4,1,2,6,"Einsteckteil LME","EN 1147",3,"",null,0]
[4,1,3,1,"Klappleiter KL","EN 1147",10,"",null,0]
[4,1,4,1,"Hakenleiter Holz HLA","EN 1147",12,"",null,0]
[4,1,4,2,"Hakenleiter Leichtmetall HLMA","EN 1147",11,"",null,0]
[4,1,5,1,"Strickleiter min. 7 m","",10,"",null,0]
[4,1,5,2,"Steckstrickleiter 10m","",8,"",null,0]
[4,1,6,1,"Multifunktionsleiter MFL","EN 1147",25,"",null,0]
[4,2,1,1,"Sprungtuch ohne Unterstützung ST 8-PES","14151-1",20,"",null,0]
[4,2,1,2,"Sprungtuch mit Unterstützung STU 8","14151-2",35,"",null,0]
[4,2,2,1,"Sprungpolster SP 16","14151-3",55,"",null,0]
[4,2,2,2,"Sprungpolster SP 24","",85,"",null,0]
[4,3,1,1,"Rettungsboot RTB 1 mit Zubehör",14961,55,"",null,0]
[4,3,1,2,"Rettungsboot RTB 2 mit Zubehör",14961,140,"",null,0]
[4,3,2,1,"Eisschlitten Stahl (für RTB-1)","",25,"",null,0]
[4,3,2,2,"Eisschlitten Kunststoff (für RTB-2)","",35,"",null,0]
[4,4,1,1,"Tierhebegerät (je nach Umfang)","",8,"",null,0]
[4,5,1,1,"Feuerwehrleine FL 30-KF mit Beutel & Trageleine","14920 /14921",2.5,"Fangleine",null,0]
[4,5,2,1,"Auffang- und Sitzgurt","EN 361 & EN 813",2,"",null,0]
[4,5,3,1,"Dreibein mit Anschlagpunkt","EN 795",27,"Dreibock",null,0]
[4,5,4,1,"Gerätesatz Absturzsicherung","14800-17",14,"",null,0]
[4,5,5,1,"Gerätesatz Auf- und Abseilgerät (bis 30 m Höhe)","14800-16",10,"",null,0]
[4,6,1,1,"Kappmesser","",0.1,"",null,0]
[4,6,1,2,"Gurtmesser","",0.2,"",null,0]
[4,6,2,1,"Nothammer","",0.5,"",null,0]
[]
[{"$nulls":7},"Gesamtmasse der ausgewählten Ausrüstung:",null,0]

{"sheet":"A_Gruppe5","index":4,"n_rows":23,"n_cols":10,"rows_kept":23,"cut":false,"hidden":false,"merged":[[4,0,4,3]],"flags":["formulas_cached_only"]}
["Die Gruppe 5 unterteilt sich in folgende Untergruppen:"]
[5,1,null,null,"Tragen"]
[5,2,null,null,"Sanitätsgerät"]
[]
["Nr.",null,null,null,"Benennung nach Norm","nach DIN","Masse","weitere Benennungen","Anzahl","Masse"]
[5,1,1,1,"Krankentrage N","13024-1",8,null,null,0]
[5,1,1,2,"Krankentrage K","13024-2",8,null,null,0]
[5,1,2,1,"Tragetuch mit Tasche","EN1865",3.5,"Rettungstuch",null,0]
[5,1,3,1,"Vakuummatratze ","",4,null,null,0]
[5,1,4,1,"Krankentransporthängematte",13023,20,null,null,0]
[5,1,5,1,"Schleifkorbtrage, Kunststoff","",13,null,null,0]
[5,1,5,2,"Hubgeschirr für Schleifkorbtrage","",2,null,null,0]
[5,1,6,1,"Rettungsbrett mit Spanngurten","",8,null,null,0]
[5,1,7,1,"Schaufeltrage","",9,null,null,0]
[5,2,1,1,"Verbandskasten K","14142",6.2,null,null,0]
[5,2,1,2,"Verbandskasten B",13164,1.5,"Kfz-Verbandkasten",null,0]
[5,2,2,1,"Notfalltasche oder -rucksack","13155",15,null,null,0]
[5,2,3,1,"Krankenhausdecke in Schutzhülle","",2.1,null,null,0]
[5,2,4,1,"Immobilisationskragen (Stifneck)","",0.1,null,null,0]
[5,2,5,1,"Kunststoff-Folie schwarz (Leichentuch)","",0.5,null,null,0]
[5,2,5,2,"Leichensack","",0.5,null,null,0]
[]
[{"$nulls":7},"Gesamtmasse der ausgewählten Ausrüstung:",null,0]

{"sheet":"A_Gruppe6","index":5,"n_rows":86,"n_cols":10,"rows_kept":86,"cut":false,"hidden":false,"merged":[[7,0,7,3]],"flags":["formulas_cached_only"]}
["Die Gruppe 6 unterteilt sich in folgende Untergruppen:"]
[6,1,null,null,"Beleuchtungsgerät"]
[6,2,null,null,"Leitungen und Zubehör"]
[6,3,null,null,"Signal- und Warngerät"]
[6,4,null,null,"Drahtloses Fernmeldegerät (Funk) und Zubehör"]
[6,5,null,null,"Drahtgebundenes Fernmeldegerät und Zubehör"]
[]
["Nr.",null,null,null,"Benennung nach Norm","nach DIN","Masse","weitere Benennungen","Anzahl","Masse"]
[6,1,1,1,"Handscheinwerfer Ex",14642,2.1,"",null,0]
[6,1,1,2,"Ladegerät für Handscheinwerfer 12/24V","",1,"",null,0]
[6,1,2,1,"Handlampe nach Wahl des Bestellers","",1,"",null,0]
[6,1,3,1,"Kopfleuchte","",2,"Helmlampe",null,0]
[6,1,4,1,"Arbeitsstellen-Scheinwerfer A250",14644,4,"",null,0]
[6,1,4,2,"Arbeitsstellen-Scheinwerfer A200",14644,3.5,"",null,0]
[6,1,4,3,"Arbeitsstellen-Scheinwerfer Xenon ",null,2,"AS 200 Xenon",null,0]
[6,1,5,1,"Breitstrahl-Scheinwerfer 110","",3,"",null,0]
[6,1,6,1,"Flutlichtstrahler 1000 Watt","",5,"",null,0]
[6,1,6,2,"Flutlichtstrahler 1500 Watt","",7,"",null,0]
[6,1,6,3,"Flutlichtstrahler Sonderleuchtmittel mind. 400 Watt",null,22,null,null,0]
[6,1,7,1,"Ballonleuchte Halogen mind. 1000 Watt",null,9,null,null,0]
[6,1,7,2,"Ballonleuchte Sonderleuchtmittel mind. 1000 Watt",null,22,null,null,0]
[6,1,8,1,"Kabelleuchte mit Lampe ex","",5,"",null,0]
[6,1,8,2,"Leuchtstoff Handleuchte 8 Watt","",0.5,"",null,0]
[6,2,1,1,"Gelenkstück D24",14640,1.7,"",null,0]
[6,2,2,1,"Stativ ca. 1,8 m",14683,5,"Dreibeinstativ ausziehbar",null,0]
[6,2,2,2,"Stativ mit Sturmverspannung mind. 3,5 m",null,16,"Teleskop-Dreibeinstativ",null,0]
[6,2,3,1,"Leitungsroller 400 V, 40 m, 1x400 V 32 A, 2x400 V 16 A, 1x250 V 16 A","EN 61316",36,"Kabeltrommel",null,0]
[6,2,3,2,"Leitungsroller 400 V, 50 m, 1x400 V, 3x250 V Dosen","EN 61316",28,"Kabeltrommel",null,0]
[6,2,3,3,"Leitungsroller 250 V, 50 m, 3x250 V Dosen","EN 61316",20,"Kabeltrommel",null,0]
[6,2,3,4,"Leitungsroller 400 V, CEE ex, 30 m, 1x400 V CEE ex","EN 61316",22,"Kabeltrommel",null,0]
[6,2,3,5,"Leitungstrommel A1-3 x 2,5-45",14680,21,"",null,0]
[6,2,3,6,"Leitungstrommel A2-3 x 2,5-95",14680,35,"",null,0]
[6,2,3,7,"Leitung HO7RN-F5G2,5, 45 m lang, ex ","",24,"",null,0]
[6,2,3,8,"Leitungstrommel K 2x4-25 (Kleinspannung)",14680,9,"",null,0]
[6,2,4,1,"Aufnahmebrücke für 2 Flutlichtstrahler",14640,1,"",null,0]
[6,2,5,1,"Abzweigstück, 3-fach","",1.4,"",null,0]
[6,2,5,2,"Schutzkontakt Stromverteiler 230 V \"Deltabox\"","",1.5,"",null,0]
[6,2,5,3,"Stromverteiler ex, 1x400 V CEE ex, 2x250 V CEE ex",null,8,null,null,0]
[6,2,5,4,"Elektro-Zwischenverteiler 400 / 230 V","",5,"Baustellenverteiler",null,0]
[6,2,6,1,"Adapterleitung 2,5m (Phasenwender)","",2.1,"",null,0]
[6,2,7,1,"Kasten mit Ersatzlampen","",1.2,"",null,0]
[6,2,8,1,"Leitung 230 V, 10 m","",3.1,"",null,0]
[6,2,9,1,"Fehlerstrom-Schutzschalter 230 V, 16 A","",0.5,"",null,0]
[6,3,1,1,"Warndreieck StVZO","",2.1,"",null,0]
[6,3,2,1,"Warnleuchte StVZO","",1,"",null,0]
[6,3,3,1,"Warnflagge 500 mm x 500 mm","",0.25,"",null,0]
[6,3,4,1,"Anhaltestab, beleuchtet, beidseitig rot leuchtend","",0.7,"Winkerkelle",null,0]
[6,3,5,1,"Verkehrswarngerät mit beidseitigem Lichtaustritt mind. 150 mm","",3.5,"Blitzleuchte",null,0]
[6,3,6,1,"Starklichtfackel ","",0.5,"",null,0]
[6,3,7,1,"Verkehrsleitkegel 500 mm nach BAST","",2.8,"",null,0]
[6,3,7,2,"Verkehrsleitkegel 750 mm nach BAST","",5.8,"",null,0]
[6,3,7,3,"Falt-Verkehrsleitkegel","",1.5,"",null,0]
[6,3,8,1,"Leitkegelleuchte","",2,"",null,0]
[6,3,9,1,"Halter (Einschlagstange) für Absperrband 1000 mm lang","",1.2,"",null,0]
[6,3,9,2,"Fuss-Ständer für Einschlagstange, verzinkt","",2,"",null,0]
[6,3,10,1,"Folienabsperrband aus PE 500 m","",2,"",null,0]
[6,3,11,1,"Absperrkette Kunststoff, 100 m","",7,"",null,0]
[6,3,12,1,"Halter aus T-Stahl 1200mm","",2.3,"",null,0]
[6,3,13,1,"Warnschild \"radioaktive Stoffe\"","",0.5,"",null,0]
[6,3,13,2,"Warnschild \"giftige Stoffe\"","",0.5,"",null,0]
[6,3,13,3,"Warnschild \"Explosionsgefahr\"","",0.5,"",null,0]
[6,3,13,4,"Warnschild \"Gefahrenstelle\"","",0.5,"",null,0]
[6,3,13,5,"Zeichen 250 \"Verbot für Fahrzeuge aller Art\"","",1,"",null,0]
[6,3,14,1,"Ständer für Warnschild mit Fuß","",5,"",null,0]
[6,3,15,1,"Faltsignal 700 mm","",2.5,"",null,0]
[6,3,15,2,"Faltsignal 900 mm","",5,"",null,0]
[6,4,1,1,"Meldertasche","",1,"",null,0]
[6,4,2,1,"Handlautsprecher mit Verstärker und Mikrofon","",2,"",null,0]
[6,4,3,1,"2-m-Handfunkgerät nach TR BOS","",1,"",null,0]
[6,4,4,2,"Ladegerät für Handsprechfunkgerät","",1,"",null,0]
[6,5,1,1,"Kopfsprechgarnitur mit Sende-Fußtaste","",0.5,"",null,0]
[6,5,2,1,"Zweibereich-Antenne für 2m- und 4m-Bereich","",0,"",null,0]
[6,5,3,1,"Antenne für 4m-Bereich","",0,"",null,0]
[6,5,4,1,"Verteilerschaltpult","",0,"",null,0]
[6,5,5,1,"Fernsprechapparat","",5,"",null,0]
[6,5,6,1,"Leitungstrommel, 30-adrig, 25 m","",0,"",null,0]
[6,5,6,2,"Spulen mit je 100 m Schaltdraht","",0,"",null,0]
[6,5,7,1,"Antennenleitung 20 m","",0,"",null,0]
[6,5,7,2,"Antennenleitung 10 m","",0,"",null,0]
[6,5,8,1,"Adapter Stecker7/16 - Kupplung N","",0,"",null,0]
[6,5,9,1,"Kabeltrommel für Feldfernsprechen","",10,"",null,0]
[6,5,9,2,"Fernsprech-Feldkabel","",0,"",null,0]
[6,5,9,3,"Rückentrage für Kabeltrommel","",4.6,"",null,0]
[6,5,10,1,"Vielfachmeßgerät und Kleinwerkzeug","",6.5,"",null,0]
[]
[{"$nulls":7},"Gesamtmasse der ausgewählten Ausrüstung:",null,0]

{"sheet":"A_Gruppe7","index":6,"n_rows":168,"n_cols":10,"rows_kept":168,"cut":false,"hidden":false,"merged":[[13,0,13,3]],"flags":["formulas_cached_only"]}
["Die Gruppe 7 unterteilt sich in folgende Untergruppen:"]
[7,1,null,null,"Hebezeuge, hydraulische und pneumatische Rettungsgeräte mit Zubehör"]
[7,2,null,null,"Seile, Leinen, Anschlagmittel"]
[7,3,null,null,"Pumpen"]
[7,4,null,null,"Stromerzeuger"]
[7,5,null,null,"Be- und Entlüftungsgeräte mit Zubehör"]
[7,6,null,null,"Motorbetriebene Arbeitsgeräte"]
[7,7,null,null,"Hölzer mit Zubehör"]
[7,8,null,null,"Auffahrbohlen, Sandbleche"]
[7,9,null,null,"Einreißhaken"]
[7,10,null,null,"Mulde"]
[7,11,null,null,"Sonstiges Arbeitsgerät"]
[]
["Nr.",null,null,null,"Benennung nach Norm","nach DIN","Masse","weitere Benennungen","Anzahl","Masse"]
[7,1,1,1,"Hebebaum 3m","",12,"Wuchtbaum",null,0]
[7,1,2,1,"Baustütze 1,7 bis 3 m","EN 1065",17,"",null,0]
[7,1,3,1,"Kanalstrebe 1,1 bis 1,4 m","4124",5.5,"",null,0]
[7,1,3,2,"Kanalstrebe 0,8 bis 1,1 m","4124",4.6,"",null,0]
[7,1,3,3,"Kanalstrebe 0,6 bis 0,9 m","4124",4,"",null,0]
[7,1,4,1,"Windenstütze, 0,6 - 1 m",null,9,null,null,0]
[7,1,4,2,"Windenstütze, 1 - 1,7 m",null,13,null,null,0]
[7,1,4,2,"Windenstütze, 1,7 - 3 m",null,18,null,null,0]
[7,1,5,1,"Hakenkette mit Verkürzungsklaue","",13.5,"",null,0]
[7,1,5,2,"Anschlagkette einsträngig mit Verkürzungsklaue, 65 kN, 4 m","",24,"",null,0]
[7,1,6,1,"Stahlwinde A 5","",25,"Zahnstangenwinde",null,0]
[7,1,6,2,"Stahlwinde A 10","",50,"Zahnstangenwinde",null,0]
[7,1,7,1,"Winde hydraulisch 50kN","",25,"Büffelheber",null,0]
[7,1,7,1,"Winde hydraulisch 100kN","",35,"Büffelheber",null,0]
[7,1,8,1,"Mehrzweckzug Z 16","14800-5",146,"",null,0]
[7,1,8,2,"Mehrzweckzug Z 32","14800-5",174,"",null,0]
[7,1,9,1,"Hebesatz H1","14800-6",110,"",null,0]
[7,1,9,2,"Hebesatz H2","14800-6",60,"",null,0]
[7,1,10,1,"Rettungsplattform, höhenverstellbar (max. 2000 x 900 x 450)","",60,"Arbeitsplattform",null,0]
[7,1,11,1,"Lufthebersatz LH 30 S ","",40,"Hebekissen, Niederdruck",null,0]
[7,1,12,1,"Hebekissen, Hochdruck, Hubkraft ca. 100 kN","E DIN EN 13731",5,"",null,0]
[7,1,12,2,"Hebekissen, Hochdruck, Hubkraft ca. 120 kN","E DIN EN 13731",6,"",null,0]
[7,1,12,3,"Hebekissen, Hochdruck, Hubkraft ca. 180 kN","E DIN EN 13731",8.5,"",null,0]
[7,1,12,4,"Hebekissen, Hochdruck, Hubkraft ca. 240 kN","E DIN EN 13731",12,null,null,0]
[7,1,12,5,"Hebekissen, Hochdruck, Hubkraft ca. 310 kN","E DIN EN 13731",17,null,null,0]
[7,1,12,6,"Hebekissen, Hochdruck, Hubkraft ca. 400 kN","E DIN EN 13731",20,null,null,0]
[7,1,12,7,"Hebekissen, Hochdruck, Hubkraft ca. 450 kN","E DIN EN 13731",26,null,null,0]
[7,1,12,8,"Hebekissen, Hochdruck, Hubkraft ca. 680 kN","E DIN EN 13731",39,null,null,0]
[7,1,13,1,"Hebekissen-Zubehörkasten - HZK","14800-11",67,"",null,0]
[7,1,14,1,"Druckgasflasche für Hebekissen 6L/300 bar","3171",11.5,"",null,0]
[7,1,15,1,"Spreizer AS (SP35) (o. Aggregat)","EN13204",20,"",null,0]
[7,1,15,2,"Spreizer BS (SP40/SP60) (o. Aggregat)","EN13204",25,"",null,0]
[7,1,15,3,"Spreizer CS (SP80) (o. Aggregat)","EN13204",30,"",null,0]
[7,1,16,1,"Schneidgerät AC (S150) (o. Aggregat)","EN13204",10,"",null,0]
[7,1,16,2,"Schneidgerät BC (S180) (o. Aggregat)","EN13204",15,"",null,0]
[7,1,16,3,"Schneidgerät CC (S200) (o. Aggregat)","EN13204",20,"",null,0]
[7,1,17,1,"Kombi-Gerät AK (o. Aggregat)","EN13204",13,"",null,0]
[7,1,17,2,"Kombi-Gerät BK (o. Aggregat)","EN13204",16,"",null,0]
[7,1,17,3,"Kombi-Gerät CK (o. Aggregat)","EN13204",19,"",null,0]
[7,1,18,1,"Rettungszylinder RZ-1","EN13204",12,"",null,0]
[7,1,18,2,"Rettungszylinder RZ-2","EN13204",16,"",null,0]
[7,1,18,3,"Rettungszylinder RZ-3","EN13204",20,"",null,0]
[7,1,19,1,"Teleskoprettungszylinder RTZ Größe 1, ca. 750 mm","EN13204",13,"",null,0]
[7,1,19,2,"Teleskoprettungszylinder RTZ Größe 2, ca. 1100 mm","EN13204",17,null,null,0]
[7,1,19,3,"Teleskoprettungszylinder RTZ Größe 3, ca. 1500 mm","EN13204",21,null,null,0]
[7,1,20,1,"Hydraulikaggregat mit Elektromotor und Schnellangriffshaspel","EN13204",85,"",null,0]
[7,1,20,2,"Hydraulikaggregat mit Verbrennungsmotor und Schnellangriffshaspel","EN13204",80,"",null,0]
[7,1,20,3,"Hydraulikkompaktaggregat mit Verbrennungsmotor","EN13204",25,"",null,0]
[7,1,20,4,"Hydraulikkompaktaggregat mit Elektromotor","EN13204",25,null,null,0]
[7,1,21,1,"Schnellangriffshaspel für hydr. Rettungsgeräte 1x20 m","",25,"",null,0]
[7,1,21,2,"Schnellangriffsdoppelhaspel für hydr. Rettungsgeräte 2x20 m","",40,"",null,0]
[7,1,21,3,"Schnellangriffsdreifachhaspel für hydr. Rettungsgeräte 3x20 m",null,110,null,null,0]
[7,1,22,1,"Schwelleraufsatz für Rettungszylinder","",10,"",null,0]
[7,1,23,1,"Stabilisierungssatz (Abstützsystem)",null,40,null,null,0]
[7,1,24,1,"Formholz in Transportkästen Größe 1","",24,"",null,0]
[7,1,25,1,"Formteile zum Unterbauen von Fahrzeugen","",10,"",null,0]
[7,1,26,1,"Airbagsicherungssystem für Fahrer",null,2,null,null,0]
[7,1,27,1,"Airbagsicherungssystem für Beifahrer",null,4,null,null,0]
[7,2,1,1,"Bindestrang 2m","",0.1,"",null,0]
[7,2,1,2,"Bindestrang 4m","",0.2,"",null,0]
[7,2,2,1,"Seil 16-FE-znk, 10 m mit Vollkauschen","",10,"Drahtseil, Stropp, Anschlagseil",null,0]
[7,2,3,1,"Seil 16-FE-znk, 2,5 m mit Ösen","",3,"Drahtseil, Stropp, Anschlagseil",null,0]
[7,2,3,2,"Seil 16-FE-znk, 5 m mit Ösen","",5,"Drahtseil, Stropp, Anschlagseil",null,0]
[7,2,3,3,"Seil 16-FE-znk, 10 m mit Ösen","",10,"Drahtseil, Stropp, Anschlagseil",null,0]
[7,2,3,4,"Seil 16-FE-znk, 20 m mit Ösen","",20,"Drahtseil, Stropp, Anschlagseil",null,0]
[7,2,4,1,"Seil 24-FE-znk, 10 m mit Vollkauschen","",23,"Drahtseil, Stropp, Anschlagseil",null,0]
[7,2,5,1,"Seil 24-FE-znk, 2,5 m mit Ösen","",6,"Drahtseil, Stropp, Anschlagseil",null,0]
[7,2,5,2,"Seil 24-FE-znk, 5 m mit Ösen","",11.5,"Drahtseil, Stropp, Anschlagseil",null,0]
[7,2,5,3,"Seil 24-FE-znk, 10 m mit Ösen","",23,"Drahtseil, Stropp, Anschlagseil",null,0]
[7,2,5,4,"Seil 24-FE-znk, 20 m mit Ösen","",46,"Drahtseil, Stropp, Anschlagseil",null,0]
[7,2,6,1,"Drahtseilklemme 16","",0.2,"",null,0]
[7,2,7,1,"Kantenreiter mit mind. 3 Umlenkrollen, 50 kN","",7,"",null,0]
[7,2,8,1,"Umlenkrolle 100kN","",25,"",null,0]
[7,2,9,1,"Schäkel Form C 1,6, 50 kN",82101,0.8,"",null,0]
[7,2,9,2,"Schäkel Form C 3,100 kN",82101,2,"",null,0]
[7,2,9,3,"Schäkel Form C 5,160 kN",82101,4.4,"",null,0]
[7,2,9,4,"Schäkel Form A 1",82101,0.8,"",null,0]
[7,2,9,5,"Schäkel Form A 3",82101,1.8,"",null,0]
[7,2,10,1,"Durchzugnadel 1800mm","",1.5,"",null,0]
[7,2,11,1,"Bindedraht 10 m","",0.3,"",null,0]
[7,2,12,1,"Polyester Rundschlinge 4 t, Nutzlänge 4 m ","EN1492-2",3.5,"Schlupf",null,0]
[7,2,13,1,"Polyester Rundschlinge 10 t, Nutzlänge 3 m ","EN1492-2",13.2,"Schlupf",null,0]
[7,2,13,2,"Polyester Rundschlinge 10 t, Nutzlänge 5 m ","EN1492-2",22,"Schlupf",null,0]
[7,2,14,1,"Zurrgurt mit Ratsche, Belastung 2500 kg, Nutzlänge 5 m","EN 12195-2",2.5,"Ratschengurt",null,0]
[7,2,14,2,"Zurrgurt mit Ratsche, Belastung 2500 kg, Nutzlänge 8 m","EN 12195-2",3.5,"Ratschengurt",null,0]
[7,2,14,1,"Zurrgurt mit Ratsche, Belastung 5000 kg, Nutzlänge 8 m","EN 12195-2",4.5,"Ratschengurt",null,0]
[7,2,12,1,"Paket Kabelbinder, 300 mm lang, 100 Stück","",0.5,"",null,0]
[7,2,16,1,"Rolle Paketklebeband, 50 mm x 30 m  ","",0.5,"",null,0]
[7,2,17,1,"Rolle Polyamidseil, 100 m lang ","",5,"",null,0]
[7,3,1,1,"Tragkraftspritze TS 2/5 mit Zubehör","",60,"",null,0]
[7,3,1,2,"Tragkraftspritze PFPN 6/600 mit Zubehör (TS4/5)","DIN EN 14466",100,"",null,0]
[7,3,1,3,"Tragkraftspritze PFPN 10/1000 mit Zubehör (TS8/8)","DIN EN 14466",190,"",null,0]
[7,3,2,1,"Tauchpumpe TP 4/1","14425",25,"",null,0]
[7,3,2,2,"Tauchpumpe TP 8/1","14425",40,"",null,0]
[7,3,2,3,"Tauchpumpe TP 15/1","14425",50,"",null,0]
[7,3,3,1,"Turbinentauchpumpe TTP 4,5/1/4",14426,11,"",null,0]
[7,3,3,2,"Turbinentauchpumpe TTP 7/1/6",14426,12,"",null,0]
[7,3,3,3,"Turbinentauchpumpe TTP 8/1/8",14426,18,"",null,0]
[7,3,3,4,"Turbinentauchpumpe TTP 10/1/10",14426,22,"",null,0]
[7,3,4,1,"Umfüllpumpe TUP 3-1,5 / GUP 3-1,5",14424,75,"",null,0]
[7,3,5,1,"Schmutzwasserpumpe (elektrisch), ca. 2000 l/min.",null,50,null,null,0]
[7,3,5,2,"Schmutzwasserpumpe (elektrisch), ca. 1000 l/min.",null,40,null,null,0]
[7,3,6,1,"Schmutzwasserpumpe (Verbrennungsmotor), ca. 500 l/min.",null,30,null,null,0]
[7,3,6,2,"Schmutzwasserpumpe (Verbrennungsmotor), ca. 800 l/min.",null,45,null,null,0]
[7,3,6,3,"Schmutzwasserpumpe (Verbrennungsmotor), ca. 1200 l/min.",null,60,null,null,0]
[7,3,7,1,"Handmembranpumpe","",11,"",null,0]
[7,3,8,1,"Absaugvorrichtung für Kraftstoff","",2,"",null,0]
[7,4,1,1,"Tragbarer Stromerzeuger 5 kVA Nennleist. mit Zubehör","14685",115,"",null,0]
[7,4,1,2,"Tragbarer Stromerzeuger 6,5 kVA Nennleist. mit Zubehör","14685",118,null,null,0]
[7,4,1,3,"Tragbarer Stromerzeuger 8 kVA Nennleist. mit Zubehör","14685",135,null,null,0]
[7,4,1,4,"Tragbarer Stromerzeuger 9 kVA Nennleist. mit Zubehör","14685",133,null,null,0]
[7,4,1,5,"Tragbarer Stromerzeuger 12 kVA Nennleist. mit Zubehör","14685",150,null,null,0]
[7,4,1,6,"Tragbarer Stromerzeuger, 13 kVA Nennleist. mit Zubehör","14685",150,null,null,0]
[7,4,1,7,"Tragbarer Stromerzeuger, 14 kVA Nennleist. mit Zubehör","14685",150,null,null,0]
[7,5,1,1,"Be- und Entlüftungsgerät 150m³/min ex m. Zubehör","",120,"",null,0]
[7,5,2,1,"Überdruck-Belüftungsgerät, elektrisch","",35,"Drucklüfter",null,0]
[7,5,2,2,"Überdruck-Belüftungsgerät, elektrisch, ex",null,40,"Drucklüfter",null,0]
[7,5,3,1,"Überdruck-Belüftungsgerät, Verbrennungsmotor",null,50,"Drucklüfter",null,0]
[7,5,4,1,"Überdruck-Belüftungsgerät, wasserbetrieben",null,35,"Drucklüfter",null,0]
[7,5,5,1,"Mobiler Rauchvorhang mit Tragetasche",null,7,"Rauchverschluss",null,0]
[7,6,1,1,"Motorsäge mit Verbrennungsmotor und Zubehör","EN 608",10,"",null,0]
[7,6,1,2,"Motorsäge mit Elektromotor und Zubehör",null,5,null,null,0]
[7,6,1,3,"Motorsäge mit Verbrennungsmotor für Verbundwerkstoffe","",18,"Rettungssäge",null,0]
[7,6,2,1,"Ersatzkette für Kettensäge","",0.5,"",null,0]
[7,6,3,1,"Spaltkeil aus Aluminium, Kunststoff oder Holz","",0.5,"",null,0]
[7,6,4,1,"Trennschleifmaschine mit Verbr.-Motor","",10,"",null,0]
[7,6,4,2,"Trennschleifmaschine elektrisch, mit Zubehör","",8,"",null,0]
[7,6,5,1,"Trennscheibe für Stein, D = 230 mm","",0.3,"",null,0]
[7,6,5,2,"Trennscheibe für Stahl, D = 230 mm","",0.3,"",null,0]
[7,6,5,3,"Trennscheibe für Stein, D = 300 mm","",0.6,"",null,0]
[7,6,5,4,"Trennscheibe für Stahl, D = 300 mm","",0.6,"",null,0]
[7,6,5,5,"Trennscheibe für Alu, D = 300 mm","",0.6,"",null,0]
[7,6,5,6,"Trennscheibe mit Diamantbesatz, D = 300 mm","",0.8,"",null,0]
[7,6,6,1,"Trenngerät mit gegenläufig rotierenden Sägeblättern mit Zubehör","",7.5,"Zwillingstrennsäge",null,0]
[7,6,7,1,"Schlagbohrmaschine m. Zubehör","",5,"",null,0]
[7,6,8,1,"Satz Bohrer","",0.3,"",null,0]
[7,6,9,1,"Akku-Schrauber","",2.5,"",null,0]
[7,6,10,1,"Bohr- und Abbruchhammer, 230 V","",12,"",null,0]
[7,6,11,1,"Säbelsäge elektr. 230 V","",4,"",null,0]
[7,7,1,1,"Transportrolle 80x5x1000 Stahl","",9.3,"",null,0]
[7,7,2,1,"Bohle mit Stahlklammern 50x220x2000-Fi",4071,14,"",null,0]
[7,7,2,2,"Unterlegbohle Hartholz 40x350x350","",4,"",null,0]
[7,7,3,1,"Kantholz, 120x160x2000-Fi",21321,23.5,"",null,0]
[7,7,4,1,"Keil aus Hartholz","",1,"",null,0]
[7,7,5,1,"Bauklammer DIN 7961-A","",0.7,"",null,0]
[7,7,5,2,"Bauklammer DIN 7961-C","",0.7,"",null,0]
[7,8,1,1,"Auffahrbohle A",14854,14,"",null,0]
[7,8,2,1,"Sandbleche aus Alu, ca. 1500 x 400 mm","",5,"",null,0]
[7,9,1,1,"Einreißhaken 2,5 einteilig","14851",5,"",null,0]
[7,9,1,2,"Einreißhaken 5 zweiteilig","",8.5,"",null,0]
[7,10,1,1,"Mulde Stahl, Edelstahl, LM","14060",6,"",null,0]
[7,11,1,1,"Industriesauger für Flüssigkeiten m. Zubehör","",35,"",null,0]
[]
[{"$nulls":7},"Gesamtmasse der ausgewählten Ausrüstung:",null,0]

{"sheet":"A_Gruppe8","index":7,"n_rows":143,"n_cols":10,"rows_kept":143,"cut":false,"hidden":false,"merged":[[10,0,10,3]],"flags":["formulas_cached_only"]}
["Die Gruppe 8 unterteilt sich in folgende Untergruppen:"]
[8,1,null,null,"Handwerksgerät"]
[8,2,null,null,"Arbeitsgeräte nicht funkenreißend"]
[8,3,null,null,"Kästen für die Feuerwehr"]
[8,4,null,null,"Thermische Trenngeräte"]
[8,5,null,null,"Mess- und Warngeräte für Gase, Chemikalien, Elektrizität, Wärme und Entfernung"]
[8,6,null,null,"Sonstiges Handwerksgerät"]
[8,7,null,null,"Öl- und Gefahrstoffgeräte"]
[8,8,null,null,"Dübel, Nägel und Schrauben"]
[]
["Nr.",null,null,null,"Benennung nach Norm","nach DIN","Masse","weitere Benennungen","Anzahl","Masse"]
[8,1,1,1,"Brechwerkzeug BaWü",14901,8.5,null,null,0]
[8,1,2,1,"Brechstange 700",14853,3.5,null,null,0]
[8,1,2,2,"Brechstange 1200",14853,6.5,null,null,0]
[8,1,2,3,"Brechstange 1500",14853,8,null,null,0]
[8,1,3,1,"Nageleisen, mind. 740 mm lang","",1,null,null,0]
[8,1,4,1,"Blechaufreißer","",2,null,null,0]
[8,1,5,1,"Holzhammer B80","",0.7,null,null,0]
[8,1,6,1,"Hammer 500S (Schlosserhammer)",1041,0.5,null,null,0]
[8,1,6,2,"Hammer 1000S (Schlosserhammer)",1041,1.1,null,null,0]
[8,1,6,3,"Hammer A5S (Vorschlaghammer)",1042,5.5,null,null,0]
[8,1,6,4,"Fäustel 2S",6475,2.3,null,null,0]
[8,1,6,5,"Hammer A570 (Latthammer)",7239,1.5,null,null,0]
[8,1,7,1,"Feuerwehraxt FA","14900",2.8,null,null,0]
[8,1,8,1,"Axt B2 SB-A","7294",2.6,null,null,0]
[8,1,9,1,"Beil 600",5131,0.8,null,null,0]
[8,1,10,1,"Zugsäge 1200",11609,1.5,null,null,0]
[8,1,11,1,"Stichsäge B 350",7258,0.3,null,null,0]
[8,1,12,1,"Bügelsäge BY oder BX","20127",1.5,null,null,0]
[8,1,12,2,"Bügelsäge 400mm",20141,1.2,null,null,0]
[8,1,13,1,"Fuchsschwanz 600",7274,1.5,null,null,0]
[8,1,14,1,"Geräte zum Trennen von Verbundglasscheiben","",1,null,null,0]
[8,1,15,1,"Drahtschere mit Fanghaken","",3,null,null,0]
[8,1,16,1,"Bolzenschneider bis 12 mm Durchmesser","",3,null,null,0]
[8,1,17,1,"Kombi-Zange 180",5244,0.4,null,null,0]
[8,1,18,1,"Flachmeißel A 300",6453,1,null,null,0]
[8,1,18,2,"Schrotmeißel",5107,2,null,null,0]
[8,1,19,1,"Schraubendreher A 0,8 x 5,5",5265,0.1,null,null,0]
[8,1,19,2,"Schraubendreher A 1 x 10",5265,0.2,null,null,0]
[8,1,20,1,"Spaten 850, mit Griffstiel CY 900 ","20127",2,null,null,0]
[8,1,21,1,"Klapp-Hackspaten","",1.5,null,null,0]
[8,1,22,1,"Kreuzhacke 3,5 mit Hackenstiel 950-76-B ",20109,4.5,null,null,0]
[8,1,23,1,"Dunggabel mit ca. 1200 mm langem Stiel",20151,1.9,null,null,0]
[8,1,24,1,"Dunghacke mit Stiel",20152,2,null,null,0]
[8,1,25,1,"Stechschaufel 5 mit Schaufelstiel","20121",2.1,"Frankfurter Schaufel",null,0]
[8,1,25,2,"Sandschaufel mit Schaufelstiel",20120,1.8,"Holsteiner Schaufel",null,0]
[8,1,26,1,"Stoßbesen mit Stiel, 1400 mm lang","",1.5,null,null,0]
[8,2,1,1,"Wasserpumpenzange B 240, nicht funkenreißend","ähnl. 5231",0.8,null,null,0]
[8,2,2,1,"Eckrohrzange 2\", nicht funkenreißend",null,2.5,null,null,0]
[8,2,3,1,"Flachmeißel A 300 nicht funkenreißend","",1,null,null,0]
[8,2,4,1,"Kupferhammer 1000S","",1.1,null,null,0]
[8,2,5,1,"Kreuzhacke 3 nicht funkenreißend","ähnl. 20109",5,null,null,0]
[8,2,6,1,"Randschaufeln nicht funkenreißend","ähnl. 20123",2.5,null,null,0]
[8,2,7,1,"Spaten, nicht funkenreißend",20127,3,null,null,0]
[8,2,8,1,"Universal-Fassschlüssel ex, 400 mm","",1.3,null,null,0]
[8,3,1,1,"Kasten DIN 14880-1-LM",14880,8,null,null,0]
[8,3,1,2,"Kasten DIN 14880-2-LM",14880,6.5,null,null,0]
[8,3,1,3,"Kasten DIN 14880-3-LM",14880,7.5,null,null,0]
[8,3,1,4,"Kasten DIN 14880-4-LM",14880,6.5,null,null,0]
[8,3,1,5,"Kasten DIN 14880-5-LM",14880,7.5,null,null,0]
[8,3,1,6,"Kasten DIN 14880-6-LM",14880,10,null,null,0]
[8,3,2,1,"Kasten DIN 14880-1-LM-O (ohne Deckel)",14880,6,null,null,0]
[8,3,2,2,"Kasten DIN 14880-2-LM-O (ohne Deckel)",14880,4.5,null,null,0]
[8,3,2,3,"Kasten DIN 14880-3-LM-O (ohne Deckel)",14880,5.5,null,null,0]
[8,3,2,4,"Kasten DIN 14880-4-LM-O (ohne Deckel)",14880,4.5,null,null,0]
[8,3,2,5,"Kasten DIN 14880-5-LM-O (ohne Deckel)",14880,5.5,null,null,0]
[8,3,2,6,"Kasten DIN 14880-6-LM-O (ohne Deckel)",14880,7.5,null,null,0]
[8,3,3,1,"Kasten DIN 14880-1-LM-O-G (ohne Deckel, gelocht)",14880,3.5,null,null,0]
[8,3,3,2,"Kasten DIN 14880-2-LM-O-G (ohne Deckel, gelocht)",14880,2.5,null,null,0]
[8,3,3,3,"Kasten DIN 14880-3-LM-O-G (ohne Deckel, gelocht)",14880,3,null,null,0]
[8,3,3,4,"Kasten DIN 14880-4-LM-O-G (ohne Deckel, gelocht)",14880,2,null,null,0]
[8,3,3,5,"Kasten DIN 14880-5-LM-O-G (ohne Deckel, gelocht)",14880,2.5,null,null,0]
[8,3,3,6,"Kasten DIN 14880-6-LM-O-G (ohne Deckel, gelocht)",14880,4.5,null,null,0]
[8,3,4,1,"Werkzeugkasten aus Stahlblech 3-teilig","",3.4,null,null,0]
[8,3,4,2,"Werkzeugkasten aus Stahlblech 5-teilig","",4.5,null,null,0]
[8,3,5,1,"Werkzeugsatztasche aus Leder od. Kunstst.","",5.9,null,null,0]
[8,3,6,1,"Tasche mit Fernmeldewerkzeug","",4,null,null,0]
[8,3,7,1,"Feuerwehr-Werkzeugkasten",14881,37,null,null,0]
[8,3,8,1,"Feuerwehr-Elektrowerkzeugkasten",14885,9.5,null,null,0]
[8,3,9,1,"Schornstein-Werkzeugkasten - SSWK","14800-4",21,null,null,0]
[8,3,10,1,"Werkzeugkasten \"Holz\" - WKH","14800-9",24,null,null,0]
[8,3,11,1,"Werkzeugkasten \"Metall I\" - WKM 1","14800-9",23,null,null,0]
[8,3,11,2,"Werkzeugkasten \"Metall II\" - WKM 2","14800-9",15,null,null,0]
[8,3,12,1,"Dichtungskasten - DK","14800-10",15,null,null,0]
[8,3,13,1,"Sperrwerkzeugkasten - SWK","14800-12",13,null,null,0]
[8,3,14,1,"Verkehrsunfallkasten - VUK","14800-13",20,null,null,0]
[8,3,15,1,"Verbrauchsmaterialkasten - VMK","14800-14",25,null,null,0]
[8,3,16,1,"Umweltschadenkasten - USK","14800-15",25,null,null,0]
[8,4,1,1,"Brennschneidgerät, tragbar","14800-7",38,null,null,0]
[8,4,2,1,"Sauerstoff-Flasche 5 Liter","",7.5,null,null,0]
[8,4,3,1,"Azetylen-Flasche 5 Liter","",10.5,null,null,0]
[8,4,4,1,"Plasmaschneidgerät, T=20 mm, mit Zubehör, IP44","",26,null,null,0]
[8,4,4,2,"Plasmaschneidgerät, T=35 mm, mit Zubehör, IP44",null,35,null,null,0]
[8,5,1,1,"Vielfach-Meßgerät (Multimeter)","",0.5,null,null,0]
[8,5,2,1,"Schutzleiter-Prüfgerät","",0.5,null,null,0]
[8,5,3,1,"Gasspürgerät","",2.5,"Prüfröhrchenpumpe",null,0]
[8,5,4,1,"Strahlenschutz Meßgerätesatz",null,7,null,null,0]
[8,5,5,1,"Kontaminations-Nachweisgerät",null,2.5,null,null,0]
[8,5,6,1,"Gaswarngerät",null,2,null,null,0]
[8,5,7,1,"Gasmessgerät",null,2,"Mehrfachgasmessgerät",null,0]
[8,5,8,1,"Fernthermometer",null,1.5,null,null,0]
[8,5,9,1,"Entfernungsmessgerät",null,1,null,null,0]
[8,5,10,1,"Gerätesatz zur Probeentnahme",null,17,null,null,0]
[8,5,11,1,"Explosionsgrenzenwarngerät","",5,"Ex-Warn",null,0]
[8,5,12,1,"Wärmebildkamera mit Zubehör","",2.5,null,null,0]
[8,5,13,1,"Packung Indikatorpapier","",0.2,null,null,0]
[8,5,14,1,"Packung Öltestpapier","",0.3,null,null,0]
[8,6,1,1,"Satz Schlüssel für Aufzüge, Sperrpfosten","",3,null,null,0]
[8,6,2,1,"Öl- und Säurebinderstreuwagen",null,5,null,null,0]
[8,6,3,1,"Flachsack aus Polyethylen (Müllsack)","",0.3,null,null,0]
[8,7,1,1,"Eimer 10 l, aus nichtrostendem Stahl, ex","",3.5,null,null,0]
[8,7,2,1,"Gummischieber 500 mm breit mit Stiel","",0.7,null,null,0]
[8,7,3,1,"Abdichtbinde, 100 mm breit x 10 m lang","",1.5,"Densobinde",null,0]
[8,7,4,1,"Dichtungshanf","",1,null,null,0]
[8,7,5,1,"Dichtungskeilesatz","",12.5,null,null,0]
[8,7,6,1,"Dichtungsmasse","",5,null,null,0]
[8,7,7,1,"Dichtungspfropfensatz","",3,null,null,0]
[8,7,8,1,"Dichtungsplatte aus Schaumstoff (900 x 900)","",0.2,null,null,0]
[8,7,9,1,"Keil aus Schaumstoff","",1,null,null,0]
[8,7,10,1,"Schachtabdeckung, 750 x 750 mm","",1,null,null,0]
[8,7,11,1,"Tankbindegurt aus Markenpolyester 10m, 8kN",60060,2.5,"Zurrgurt mit Ratsche",null,0]
[8,7,12,1,"Anschlußzwinge (Messing)","",1.2,null,null,0]
[8,7,13,1,"Ausgussrohr ex","",3.5,null,null,0]
[8,7,14,1,"Rohrbogen 90°ex","",2,null,null,0]
[8,7,15,1,"Schnellschlusshahn DN 50 aus Messing","",4.6,null,null,0]
[8,7,16,1,"Saugrohr, 1100 mm lang, ex","",2.5,null,null,0]
[8,7,17,1,"Erdungsspieß aus T-Stahl, 550 mm lang","",1.5,null,null,0]
[8,7,18,1,"Haftmagnet ( für Erdungszwecke )","",0.5,null,null,0]
[8,7,19,1,"Massekabel aus Kupferlitze, 50 m lang","",13.5,null,null,0]
[8,7,20,1,"Litzentrommel",null,1.6,null,null,0]
[8,7,21,1,"Sieb- und Räumschaufel für Ölbindemittel (Lochblech)","",3,null,null,0]
[8,8,1,1,"Allzweckdübelsatz, jeweils 100 Stück","",0.5,null,null,0]
[8,8,2,1,"Einpressdübelsatz, jeweils 10 Stück","",2,null,null,0]
[8,8,3,1,"Gewindebolzensatz, M12, M16, M20","",20,null,null,0]
[8,8,4,1,"Holzschraubensatz","",1.4,null,null,0]
[8,8,5,1,"Kammnägel, Paket mit 100 Stück","",1,null,null,0]
[8,8,6,1,"Lochbleche für Nagelverbindung","",5,null,null,0]
[8,8,7,1,"Nagelsatz, 2,5 kg","",20,null,null,0]
[8,8,8,1,"Scheibensatz","",3.6,null,null,0]
[8,8,9,1,"Schnellbauschraubensatz, jew. 100 Stück","",1.8,null,null,0]
[8,8,10,1,"Sechskantmuttersatz, M12, M16, M20","",2.6,null,null,0]
[]
[{"$nulls":7},"Gesamtmasse der ausgewählten Ausrüstung:",null,0]

{"sheet":"A_Gruppe9","index":8,"n_rows":86,"n_cols":10,"rows_kept":86,"cut":false,"hidden":false,"merged":[[9,0,9,3]],"flags":["formulas_cached_only"]}
["Die Gruppe 9 unterteilt sich in folgende Untergruppen:"]
[9,1,null,null,"Fahrzeug-Zusatzgerät"]
[9,2,null,null,"Folien, Planen, Rinnen"]
[9,3,null,null,"Trichter, Schöpfer, Mulden"]
[9,4,null,null,"Gerätesatz Gefahrgut"]
[9,5,null,null,"Faltbehälter, Auffangmittel"]
[9,6,null,null,"Sonstiges Zubehör"]
[9,7,null,null,"Schnelleinsatzzelte und Duschen"]
[]
["Nr.",null,null,null,"Benennung nach Norm","nach DIN","Masse","weitere Benennungen","Anzahl","Masse"]
[9,1,1,1,"Kanister, gefüllt mit 20 Liter Kraftstoff",7274,21.5,"Ersatzkanister",null,0]
[9,1,1,2,"Kanister, gefüllt mit 10 Liter Kraftstoff",7274,10.5,"Ersatzkanister",null,0]
[9,1,2,1,"Reservekraftstoffkanister, PE, 5 l Inhalt, leer","",0.8,"Ersatzkanister",null,0]
[9,1,2,2,"Reservekraftstoffkanister, PE, 5 l Inhalt, gefüllt","",5,"Ersatzkanister",null,0]
[9,1,2,3,"Doppelkanister für Motorsäge 5 + 2 Liter","",7.8,null,null,0]
[9,1,3,1,"Ölbehälter, gefüllt mit 2 l Kettenöl","",2.5,null,null,0]
[9,1,4,1,"Ausgußstutzen flexibel für Kanister","",0.2,null,null,0]
[9,1,5,1,"Schleppstange mit Zugöse ",74054,20,"Abschleppstange",null,0]
[9,1,6,1,"Abschleppseil 16mm, 5m, Draht",76031,6.6,null,null,0]
[9,1,6,2,"Abschleppseil 3500kg - 5m, Kunststoff","",1.6,null,null,0]
[9,1,6,3,"Abschleppseil 6000kg - 5m, Kunststoff","",3.6,null,null,0]
[9,1,7,1,"Abgasschlauch 50 x 1500","14572",2.5,null,null,0]
[9,1,7,2,"Abgasschlauch 50 x 2500","14572",4,null,null,0]
[9,1,7,3,"Abgasschlauch 85 x 2500","14572",6.5,null,null,0]
[9,1,7,4,"Abgasschlauch 102 x 2500","14572",10,null,null,0]
[9,1,8,1,"Unterlegkeil A , Nenngröße 36 D, bis 1600 kg Radlast",76051,1,null,null,0]
[9,1,8,2,"Unterlegkeil A , Nenngröße 46, bis 5000 kg Radlast",76051,3.1,null,null,0]
[9,1,8,3,"Unterlegkeil A , Nenngröße 53, bis 6500 kg Radlast",76051,4.4,null,null,0]
[9,1,8,4,"Unterlegkeil Größe 1, für masch. angetr. Zugeinrichtung","14584",16,"Windenkeile",null,0]
[9,1,8,5,"Unterlegkeil Größe 2, für masch. angetr. Zugeinrichtung","",25,"Windenkeile",null,0]
[9,1,9,1,"Starthilfekabel",72551,6,null,null,0]
[9,2,1,1,"Kunststoff-Folie, 25 m lang, 4 m breit","",16.5,null,null,0]
[9,2,2,1,"Schweißgerät für Kunststoff-Folien mind. 300 mm","",8,null,null,0]
[9,2,3,1,"Abdeck- und Auffangplane, Größe 2 m x 2 m","",3,null,null,0]
[9,2,3,2,"Abdeck- und Auffangplane, Größe 4 m x 6 m","",5,null,null,0]
[9,2,4,1,"Auffangrinne Alu weich","",4,null,null,0]
[9,2,4,2,"Auffangrinne Alu halbhart","",4,null,null,0]
[9,3,5,1,"Trichter 250 mm nicht funkenreißend","",0.6,null,null,0]
[9,3,5,2,"Auffangtrichter  400 mm x 400 mm x 150 mm mit Außlaufrohr","",15,null,null,0]
[9,3,6,1,"Schöpfer aus Alu, 1l","",1,null,null,0]
[9,3,6,2,"Schöpfer aus nichtrostendem Stahl, 1l, nicht funkenreißend","",0.9,null,null,0]
[9,3,6,3,"Schöpfeimer mit Stiel aus nichtrostendem Stahl, 5 l, ex","",2.5,null,null,0]
[9,3,7,1,"Mulde LM",14060,2.7,null,null,0]
[9,3,7,2,"Mulde aus nichtrostendem Stahl",14060,7,null,null,0]
[9,4,1,1,"Ölbindemittel für den Einsatz auf Verkehrsflächen","",20,null,null,0]
[9,4,1,2,"Ölbindemittel für den Einsatz auf Gewässern","",10,null,null,0]
[9,4,2,1,"Säurebindemittel","",15,null,null,0]
[9,4,3,1,"Ölbindeschlauch 3m, 200mm","",6,null,null,0]
[9,4,4,1,"Saugtücher für Öl ca. 100 Stück (300 x 300 mm)","",2,null,null,0]
[9,4,5,1,"Ölbindeflies (Rolle) ca. 40m, 400 mm","",8.5,null,null,0]
[9,4,6,1,"Jutesack (Sandsack)","",0.4,null,null,0]
[9,4,7,1,"Bleiwolle","",2,null,null,0]
[9,4,8,1,"Lehmmehl 10kg","",10,null,null,0]
[9,4,9,1,"Leckverschlüsse formstabil mit Zubehör","",40,null,null,0]
[9,4,9,2,"Leckverschlüsse pneumatisch mit Zubehör","",10,null,null,0]
[9,4,10,1,"Tankwagenübergangsstücke (Satz)","",44,null,null,0]
[9,4,11,1,"Putzwolle","",2,null,null,0]
[9,4,11,2,"Paket Putzlappen ca. 25 Stück (50 x 50 cm)","",3,null,null,0]
[9,5,1,1,"Faltbehälter, offen, selbstaufrichtend, 3000 l","",12,"Auffangbehälter",null,0]
[9,5,1,2,"Faltbehälter, offen, selbstaufrichtend, 5000 l","",14,"Auffangbehälter",null,0]
[9,5,1,3,"Faltbehälter, offen, selbstaufrichtend, 10000 l","",25,"Auffangbehälter",null,0]
[9,5,2,1,"Faltbehälter, offen, mit Stützgerüst, 1800 l","",20,"Auffangbehälter",null,0]
[9,5,2,2,"Faltbehälter, offen, mit Stützgerüst, 3000 l","",45,"Auffangbehälter",null,0]
[9,5,3,1,"Faltbehälter, geschlossen, 1500 l","",8,"Auffangbehälter",null,0]
[9,5,3,2,"Faltbehälter, geschlossen, 3000 l","",20,"Auffangbehälter",null,0]
[9,5,3,3,"Faltbehälter, geschlossen, 5000 l","",26,"Auffangbehälter",null,0]
[9,5,3,4,"Faltbehälter, geschlossen, 10000 l","",47,"Auffangbehälter",null,0]
[9,5,4,1,"Faltbehälter, mineralölbeständig, offen, selbstaufrichtend, 1500 l","",12,"Auffangbehälter",null,0]
[9,5,4,2,"Faltbehälter, mineralölbeständig, offen, selbstaufrichtend, 3000 l","",15,"Auffangbehälter",null,0]
[9,5,4,3,"Faltbehälter, mineralölbeständig, offen, selbstaufrichtend, 5000 l","",22,"Auffangbehälter",null,0]
[9,5,5,1,"Faltbehälter, mineralölbeständig, offen, mit Stützgerüst, 3000 l","",33,"Auffangbehälter",null,0]
[9,5,6,1,"Faltbehälter, mineralölbeständig, geschlossen, 1500 l","",15,"Auffangbehälter",null,0]
[9,5,6,2,"Faltbehälter, mineralölbeständig, geschlossen, 3000 l","",21,"Auffangbehälter",null,0]
[9,5,6,3,"Faltbehälter, mineralölbeständig, geschlossen, 5000 l","",27,"Auffangbehälter",null,0]
[9,5,6,4,"Faltbehälter, mineralölbeständig, geschlossen, 10000 l","",47,"Auffangbehälter",null,0]
[9,5,7,1,"Überstülpfässer PE","",35,"Bergefass",null,0]
[9,5,7,2,"Überstülpfässer Edelstahl","",45,"Bergefass",null,0]
[9,5,8,1,"Auffangwanne PE, 200 l","",15,null,null,0]
[9,5,9,1,"Satz Behälter, Edelstahl, Ges. Volumen 2500 l, 5 Behälter mit Deckel","",135,null,null,0]
[9,5,10,2,"Einhängebehälter aus PVC (für  9.5.9.1)","",2,null,null,0]
[9,6,1,1,"Rolle Klebeband, mit Warnzeichen für Radioaktivität","",0.2,null,null,0]
[9,7,1,1,"Schnelleinsatzzelt selbstaufrichtend 4 x 5 m","",80,null,null,0]
[9,7,1,2,"Schnelleinsatzzelt selbstaufrichtend 6 x 5 m","",110,null,null,0]
[9,7,2,1,"Schnelleinsatzdusche","",35,"Dekontaminationsdusche",null,0]
[]
[{"$nulls":7},"Gesamtmasse der ausgewählten Ausrüstung:",null,0]